<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<schematic>
<libraries>
<library name="microbuilder">
<packages>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100 &lt;/b&gt;&lt;p&gt;Low Profile Quad Flat Package 14x14x1.4 mm&lt;p&gt;</description>
</package>
<package name="QFN24_4MM">
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
<package name="DO-1N4148">
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;</description>
</package>
<package name="CRYSTAL32SMT">
<description>32.768KHz Crystal - SMT Cylinder</description>
</package>
<package name="CRYSTAL_3.2X2.5">
<description>3.2mm x 2.5mm Thin SMT Crystal</description>
</package>
<package name="CRYSTAL_4.9X1.8">
<description>&lt;p&gt;4.9mm x 1.8mm Thin SMT Crystal&lt;/p&gt;
Epson Toyocom FCC-255</description>
</package>
</packages>
<symbols>
<symbol name="FRAME_A3">
</symbol>
<symbol name="LPC1768_QFP">
<pin name="TDO/SWO"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="TCK/SWDCLK"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="VREFP"/>
<pin name="N.C."/>
<pin name="RSTOUT"/>
<pin name="VREFN"/>
<pin name="RTCX1"/>
<pin name="RESET"/>
<pin name="RTCX2"/>
<pin name="VBAT"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0[28]/SCL0/USB_SCL"/>
<pin name="P0[27]/SDA0/USB_SDA"/>
<pin name="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
<pin name="P3[25]/MAT0[0]/PWM1[2]"/>
<pin name="VDD(3V3)1"/>
<pin name="P0[29]/USB_D+"/>
<pin name="P0[30]/USB_D-"/>
<pin name="VSS1"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MC0A/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCFB0/PWM1[2]/SCK0"/>
<pin name="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
<pin name="P1[22]/MC0B/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCFB1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCFB2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MC1A/MAT1[1]"/>
<pin name="P1[26]/MC1B/PWM1[6]/CAP0[0]"/>
<pin name="VSS2"/>
<pin name="VDD(REG)(3V3)1"/>
<pin name="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
<pin name="P1[28]/MC2A/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MC2B/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P2[13]/EINT3/I2STX_SDA"/>
<pin name="P2[12]/EINT2/I2STX_WS"/>
<pin name="P2[11]/EINT1/I2STX_CLK"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VDD(3V3)2"/>
<pin name="VSS3"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[21]/RI1/RD1"/>
<pin name="P0[20]/DTR1/SCL1"/>
<pin name="P0[19]/DSR1/SDA1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2"/>
<pin name="P2[8]/TD2/TXD2"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)3"/>
<pin name="VSS4"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
<pin name="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS6"/>
<pin name="VDD(REG)(3V3)2"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)4"/>
<pin name="VSS5"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
<pin name="RTCK"/>
</symbol>
<symbol name="LAN8720">
<pin name="MDIO"/>
<pin name="MDC"/>
<pin name="NINT/REFCLKO"/>
<pin name="TXD0"/>
<pin name="TXD1"/>
<pin name="TXEN"/>
<pin name="RXD0"/>
<pin name="RXD1"/>
<pin name="RXER"/>
<pin name="LED1/REGOFF"/>
<pin name="LED2/NINTSEL"/>
<pin name="NRST"/>
<pin name="TX+"/>
<pin name="TX-"/>
<pin name="RX+"/>
<pin name="RX-"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="CRS_DV"/>
<pin name="RBIAS"/>
<pin name="GND"/>
<pin name="VDD1A"/>
<pin name="VDD2A"/>
<pin name="VDDIO"/>
<pin name="VDDCR"/>
</symbol>
<symbol name="FERRITE">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="74LVC1G04">
<pin name="NC" direction="nc"/>
<pin name="A"/>
<pin name="GND" direction="pwr"/>
<pin name="Y"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FRAME_A3" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A3, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="FRAME_A3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1768" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1768 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 512 kB Flash, 64 kB SRAM, USB Device/Host/OTG, Ethernet, CAN, I2S, 10-bit DAC &lt;/p&gt;
&lt;p&gt;Digikey: 568-4796-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1768_QFP"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="N.C." pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_D+" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_D-" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MC0A/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCFB0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MC0B/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCFB1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCFB2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MC1A/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MC1B/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MC2A/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MC2B/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LAN8720" prefix="U" uservalue="yes">
<description>&lt;b&gt;LAN8720A 10/100 Ethernet PHY&lt;/b&gt;
&lt;p&gt;Mouser: 886-LAN8720AI-CP&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LAN8720"/>
</gates>
<devices>
<device name="" package="QFN24_4MM">
<connects>
<connect gate="G$1" pin="CRS_DV" pad="11"/>
<connect gate="G$1" pin="GND" pad="THERM"/>
<connect gate="G$1" pin="LED1/REGOFF" pad="3"/>
<connect gate="G$1" pin="LED2/NINTSEL" pad="2"/>
<connect gate="G$1" pin="MDC" pad="13"/>
<connect gate="G$1" pin="MDIO" pad="12"/>
<connect gate="G$1" pin="NINT/REFCLKO" pad="14"/>
<connect gate="G$1" pin="NRST" pad="15"/>
<connect gate="G$1" pin="RBIAS" pad="24"/>
<connect gate="G$1" pin="RX+" pad="23"/>
<connect gate="G$1" pin="RX-" pad="22"/>
<connect gate="G$1" pin="RXD0" pad="8"/>
<connect gate="G$1" pin="RXD1" pad="7"/>
<connect gate="G$1" pin="RXER" pad="10"/>
<connect gate="G$1" pin="TX+" pad="21"/>
<connect gate="G$1" pin="TX-" pad="20"/>
<connect gate="G$1" pin="TXD0" pad="17"/>
<connect gate="G$1" pin="TXD1" pad="18"/>
<connect gate="G$1" pin="TXEN" pad="16"/>
<connect gate="G$1" pin="VDD1A" pad="19"/>
<connect gate="G$1" pin="VDD2A" pad="1"/>
<connect gate="G$1" pin="VDDCR" pad="6"/>
<connect gate="G$1" pin="VDDIO" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE" prefix="FB" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ferrite Bead&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0603&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MMZ1608B121C - 120 Ohm, 600mA Ferrite Chip - Digikey: 445-2164-1-ND&lt;/li&gt;
&lt;li&gt;BK1608HW121-T - 120 Ohm, 600mA Ferrite Chip - Digikey: 587-1876-2-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="FERRITE"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G04" prefix="U" uservalue="yes">
<description>&lt;b&gt;74LVC1G04&lt;/b&gt; - Single Inverter Gate
&lt;p&gt;&lt;b&gt;SOT23-5&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;SN74LVC1G04DBVR - Digikey: 296-11599-1-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="74LVC1G04"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Diode&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;SMADIODE&lt;/b&gt; - SMA Surface Mount Package
&lt;ul&gt;
&lt;li&gt;20V 1A Schottky Diode Digikey (500mV @ 1A, 500uA Vr @ 20V): 641-1014-6-ND&lt;/li&gt;
&lt;li&gt;10V 2A Schottky Diode Digikey (350mV @ 2A, 700uA Vr @ 10V): MBRA210LT3&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOD-123&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;30V 200mA (800mV Vf, 2uA Vr @ 25V) Schottky Diode (very fast switching for boost, etc.) - Digikey: BAT54T1GOSTR-ND&lt;/li&gt;
&lt;li&gt;30V 500mA (430mV Vf, 130uA Vr @ 30V) Schottky Diode - Digikey: B0530W-FDICT-ND&lt;/li&gt;
&lt;li&gt;MBR120 1A 20V (0.34Vf) Schottky Diode - Digikey: MBR120VLSFT1GOSCT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOD-323&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;10V 570mA (380mV Vf, 3ns) Schottky Diode - Digikey: ZLLS410CT-ND&lt;/li&gt;
&lt;li&gt;1N4148WS - 75V 150mA (1V Vf @ 10mA, 4ns) Simple Diode - Digikey: 1N4148WSFSCT-ND, Mouser: 512-1N4148WS&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOD-523&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;BAT54 30V 200mA Schottky (0.8 Vf @ 100mA, 5ns) - Digikey: BAT54XV2CT-ND&lt;/li&gt;
&lt;li&gt;30V 30mA Schottky Diode (RB751S-40TE61) - Digikey: RB751S-40TE61CT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOT23-R/W&lt;/b&gt; - SOT23 Package (R = Solder Paste/Reflow Ovens, W = Hand-Soldering)
&lt;ul&gt;
&lt;li&gt;BAT54Film 40V 300mA - Digikey: 497-7162-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;DO-1N4148&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Through Hole Small Current Diode (any model)&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="SMA" package="SMADIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-1N4148" package="DO-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-523" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-323" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-123" package="SOD-123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Crystals&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;HC49UP&lt;/b&gt; - Surface Mount Crystal
&lt;ul&gt;
&lt;li&gt;4.0MHz 18pF +/-30ppm Surface Mount Crystal [Digikey: 535-9857-1-ND]&lt;/li&gt;
&lt;li&gt;12.0 MHz Surface Mount Crystal [Digikey: 535-9869-6-ND]&lt;/li&gt;
&lt;li&gt;25.0 MHz Surface Mount Crystal [Digikey: 535-9078-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;3.2 x 2.5mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;12.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: &lt;b&gt;-10-70°C&lt;/b&gt;: 644-1047-1-ND &lt;b&gt;-40-125°C&lt;/b&gt;: 644-1128-1-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: &lt;b&gt;-10-70°C&lt;/b&gt;: 644-1049-1-ND &lt;b&gt;-40-125°C&lt;/b&gt;: 644-1129-2-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 10pF 10ppm 3.2 x 2.5mm Crystal [Digikey: 644-1100-1-ND]&lt;/li&gt;
&lt;li&gt;27.12 MHz 18pF 30ppm 3.2 x 2.5mm Crystal [Digikey: 887-1424-1-ND]&lt;/li&gt;
&lt;li&gt;27.12MHz 10pF 10ppm 3.2 x 2.5mm Crystal [Digikey: 887-1329-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;4.9 x 1.8mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;32.768 KHz 12.5pF 20ppm 4.9 x 1.8mm Crystal [Digikey: SE2415CT-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;Cylinder&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;32.768KHz Cylinder Crystal&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="SMD" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="32.768" package="CRYSTAL32SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN" package="CRYSTAL_3.2X2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN32K" package="CRYSTAL_4.9X1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun">
<packages>
<package name="EIA3216">
</package>
<package name="EIA3528">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="EIA7343">
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="NIPPON_F80">
</package>
<package name="PANASONIC_D">
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="VISHAY_C">
</package>
<package name="PANASONIC_H13">
</package>
<package name="INDUCTOR-1206">
</package>
<package name="0603">
</package>
<package name="CR54">
</package>
<package name="CDRH125">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="B82462G">
</package>
<package name="CR75">
</package>
<package name="1210">
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="COOPER_UP4B">
</package>
<package name="CDRH3D28">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
<package name="1X06">
</package>
<package name="MOLEX-1X6">
</package>
<package name="MOLEX-1X6-RA">
</package>
<package name="1X06-SMD">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X6_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X6-RA_LOCK">
</package>
<package name="1X06-SIP_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06_FEMALE_LOCK.010">
</package>
<package name="1X06_LONGPADS">
</package>
<package name="1X06-SMD_EDGE">
</package>
<package name="SCREWTERMINAL-3.5MM-6">
</package>
<package name="1X06-SMD-FEMALE">
</package>
<package name="1X06-SMD-FEMALE-V2">
<description>Package for 4UCONN part #19686 *UNPROVEN*</description>
</package>
<package name="1X04">
</package>
<package name="MOLEX-1X4">
</package>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
<package name="1X04-1.27MM">
</package>
<package name="1X04_LOCK">
</package>
<package name="1X04_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X4_LOCK">
</package>
<package name="1X04-SMD">
</package>
<package name="1X04_LONGPADS">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="1X03">
</package>
<package name="MOLEX-1X3">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X03_LOCK">
</package>
<package name="1X03_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X3_LOCK">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="USD-SOCKET-PP">
<description>OLD Production Socket. DO NOT USE for production boards.</description>
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="POWER_JACK_SLOT">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="RCA">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="RCA_LOCK">
</package>
<package name="1206">
</package>
<package name="AXIAL-0.3">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="1X02">
</package>
<package name="MOLEX-1X2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="S2B-PH">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_BIG">
</package>
<package name="S2B-PH-VERTICAL">
</package>
<package name="R_SW_TH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LOCK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-NO-NS">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_3">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
</packages>
<symbols>
<symbol name="3.3V">
<pin name="3.3V" direction="sup"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="5V">
<pin name="5V" direction="sup"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="M04">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="USDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="RSV"/>
<pin name="DO"/>
<pin name="NC"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@1"/>
<pin name="SHIELD@2"/>
<pin name="SHIELD@4"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JUMPER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="SJ_2">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="3.3V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_POL" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor Polarized&lt;/b&gt;
These are standard SMD and PTH capacitors. Normally 10uF, 47uF, and 100uF in electrolytic and tantalum varieties. Always verify the external diameter of the through hole cap, it varies with capacity, voltage, and manufacturer. The EIA devices should be standard.</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="1206" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CPOL-RADIAL-100UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CPOL-RADIAL-10UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7343" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F80" package="NIPPON_F80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CPOL-RADIAL-1000UF-63V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="CPOL-RADIAL-1000UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="VISHAY_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H13" package="PANASONIC_H13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;
Basic Inductor/Choke - 0603 and 1206. Footprints are not proven and vary greatly between part numbers.</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="H*" package="INDUCTOR-1206">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="1206"/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR54" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PWR" package="CDRH125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B82462G" package="B82462G">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75" package="CR75">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1007" package="1007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="COOPER_UP4B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="CDRH3D28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5V">
<gates>
<gate name="G$1" symbol="5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;Momentary Switch&lt;/b&gt;
Button commonly used for reset or general input. Spark Fun Electronics SKU : COM-00097</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSA_SEALED" package="KSA_SEALED_TAC_SWITCH">
<connects>
<connect gate="S" pin="1" pad="P$1"/>
<connect gate="S" pin="2" pad="P$2"/>
<connect gate="S" pin="3" pad="P$3"/>
<connect gate="S" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 6&lt;/b&gt;
Standard 6-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08094 with associated crimp pins and housings.

NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="SIP" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX-1X6-RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIP_LOCK" package="1X06-SIP_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X06-SMD_EDGE_FEMALE" package="1X06-SMD_EDGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMDF" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE-V2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 4&lt;/b&gt;
Standard 4-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M04"/>
</gates>
<devices>
<device name="PTH" package="1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X04-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X04_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X04_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X04-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X04_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X04_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USD-SOCKET" prefix="U">
<description>&lt;b&gt;microSD Socket&lt;/b&gt;
Push-push type uSD socket. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00127. tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed).</description>
<gates>
<gate name="G$1" symbol="USDCARD"/>
</gates>
<devices>
<device name="USD" package="USD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD2"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="GND2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="MICRO-SD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND3"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="CD2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;b&gt;Power Jack&lt;/b&gt;
This is the standard 5.5mm barrel jack for power. The PTH is the most common, proven, reliable, footprint. All others are experimental. The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned. Spark Fun Electronics SKU : PRT-00119. Mating wall wart : TOL-00298 (and others)</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA" package="RCA">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RCA_LOCK" package="RCA_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="BARREL"/>
<connect gate="G$1" pin="GNDBREAK" pad="SPRING"/>
<connect gate="G$1" pin="PWR" pad="BREAK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH 1/10th watt (small) resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 2&lt;/b&gt;
Standard 2-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08233 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S2B-PH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="S2B-PH-VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO-NS" package="SJ_2S-NO-NS">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="X">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5664</description>
</package>
<package name="HPC0201">
<description>&lt;b&gt; &lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/10129/hpc0201a.pdf</description>
</package>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
<package name="C1808">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Source: AVX .. aphvc.pdf</description>
</package>
<package name="C3640">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Source: AVX .. aphvc.pdf</description>
</package>
</packages>
<symbols>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HPC0201" package="HPC0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0201" package="C0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1808" package="C1808">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3640" package="C3640">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply2">
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="GND" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="resistor">
<packages>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5664</description>
</package>
</packages>
<symbols>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="R-US_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/2V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="resistor-dil">
<packages>
<package name="0603-ARC">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
concave termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="CAT16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="CAY16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="YC124">
<description>&lt;b&gt;ARRAY CHIP RESISTOR&lt;/b&gt; Size 4 x 0402&lt;p&gt;
Source: www.yageo.com .. Pu-YC124_51_PbFree_L_1.pdf</description>
</package>
<package name="4X0402ARV341">
<description>&lt;b&gt;Array chip resistor&lt;/b&gt; size 4 × 0402&lt;p&gt;
Source: http://docs-europe.electrocomponents.com/webdocs/0114/0900766b80114d99.pdf</description>
</package>
<package name="EXB18V">
<description>&lt;b&gt;Chip Resistor Array 0201x4&lt;/b&gt; 4 resistors in 1.4 mm x 0.6 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXB28V">
<description>&lt;b&gt;Chip Resistor Array 0402x4&lt;/b&gt; 4 resistors in 2.0 mm x 1.0 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXB38V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.2 mm x 1.6 mm size (EXB38V, V8V)&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBN8V">
<description>&lt;b&gt;Chip Resistor Array 0402x4&lt;/b&gt; 4 resistors in 2.0 mm x 1.0 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBS8V">
<description>&lt;b&gt;Chip Resistor Array 0805x4&lt;/b&gt; 4 resistors in 5.08 mm x 2.20 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
<package name="EXBV8V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.20 mm x 1.60 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
</packages>
<symbols>
<symbol name="R1NV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="4R-N" prefix="RN" uservalue="yes">
<description>&lt;b&gt;Array Chip Resistor&lt;/b&gt;&lt;p&gt;
Source: RS Component / Phycomp</description>
<gates>
<gate name="A" symbol="R1NV"/>
<gate name="B" symbol="R1NV"/>
<gate name="C" symbol="R1NV"/>
<gate name="D" symbol="R1NV"/>
</gates>
<devices>
<device name="0603-ARC" package="0603-ARC">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="0603-ARV" package="0603-ARV">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="CAT16" package="CAT16">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="CAY16" package="CAY16">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="YC124" package="YC124">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="0402ARV341" package="4X0402ARV341">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXB18V" package="EXB18V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXB28V" package="EXB28V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXB38V" package="EXB38V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXBN8V" package="EXBN8V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXBS8V" package="EXBS8V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="EXBV8V" package="EXBV8V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="jumper">
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="JP2E">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="JP1E" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="JP2E"/>
</gates>
<devices>
<device name="" package="JP1">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Geos">
<packages>
<package name="TSSOP20">
</package>
<package name="MOLEX8981">
</package>
<package name="TO263AB">
</package>
</packages>
<symbols>
<symbol name="ATX_HDD">
<pin name="+12V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="MCP44X1">
<pin name="P3A"/>
<pin name="P3W"/>
<pin name="P3B"/>
<pin name="HVC/A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSS"/>
<pin name="P1B"/>
<pin name="P1W"/>
<pin name="P1A"/>
<pin name="P0A"/>
<pin name="P0W"/>
<pin name="P0B"/>
<pin name="NC"/>
<pin name="!RESET"/>
<pin name="A1"/>
<pin name="VDD"/>
<pin name="P2B"/>
<pin name="P2W"/>
<pin name="P2A"/>
</symbol>
<symbol name="ETH1506S">
<pin name="N/C"/>
<pin name="K"/>
<pin name="A"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HDD-ATX_CON" uservalue="yes">
<description>&lt;H&gt;&lt;b&gt;ATX HDD Connector 4 pin&lt;/b&gt;&lt;/h&gt;&lt;br&gt;
Molex8981 Connector</description>
<gates>
<gate name="G$1" symbol="ATX_HDD"/>
</gates>
<devices>
<device name="" package="MOLEX8981">
<connects>
<connect gate="G$1" pin="+12V" pad="P$1"/>
<connect gate="G$1" pin="+5V" pad="P$4"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="GND1" pad="P$3"/>
</connects>
<technologies>
<technology name="">
<attribute name="J" value="ATX-HDD"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP44X1">
<description>&lt;b&gt;&lt;h&gt;MCP44x1&lt;/h&gt;&lt;/b&gt;
&lt;p&gt; MCP4451 - &lt;br&gt;
? Quad Resistor Network&lt;br&gt;
? I2C Serial Interface Support&lt;br&gt;
? Potentiometer or Rheostat Configuration Options&lt;br&gt;
? Resistor Network Resolution:&lt;br&gt;
7-bit ? 128 Resistors (129 Taps)&lt;br&gt;
8-bit ? 256 Resistors (257 Taps)</description>
<gates>
<gate name="G$1" symbol="MCP44X1"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!RESET" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="HVC/A0" pad="4"/>
<connect gate="G$1" pin="NC" pad="14"/>
<connect gate="G$1" pin="P0A" pad="11"/>
<connect gate="G$1" pin="P0B" pad="13"/>
<connect gate="G$1" pin="P0W" pad="12"/>
<connect gate="G$1" pin="P1A" pad="10"/>
<connect gate="G$1" pin="P1B" pad="8"/>
<connect gate="G$1" pin="P1W" pad="9"/>
<connect gate="G$1" pin="P2A" pad="20"/>
<connect gate="G$1" pin="P2B" pad="18"/>
<connect gate="G$1" pin="P2W" pad="19"/>
<connect gate="G$1" pin="P3A" pad="1"/>
<connect gate="G$1" pin="P3B" pad="3"/>
<connect gate="G$1" pin="P3W" pad="2"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETH1506S" uservalue="yes">
<description>&lt;h&gt;&lt;b&gt; ETH1506S &lt;/b&gt; &lt;/h&gt; 
&lt;p&gt;Package : TO-263AB (D2PAK), TO-262AA &lt;br&gt;
IF(AV) : 15 A&lt;br&gt;
VR : 600 V&lt;br&gt;
Hyperfast Rectifier, 15 A FRED Pt
Diode variation Single die</description>
<gates>
<gate name="G$1" symbol="ETH1506S"/>
</gates>
<devices>
<device name="" package="TO263AB">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="K"/>
<connect gate="G$1" pin="N/C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="led">
<packages>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="SMT1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KA-3528ASYC" package="KA-3528ASYC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0805" package="SML0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML1206" package="SML1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0603" package="SML0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp-quick">
<packages>
<package name="08P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="M08">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M08" prefix="SL" uservalue="yes">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="M08"/>
</gates>
<devices>
<device name="" package="08P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="transistor-power">
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
<symbols>
<symbol name="MFNS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="IRF540" prefix="Q">
<description>&lt;b&gt;HEXFET Power MOSFET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MFNS"/>
</gates>
<devices>
<device name="" package="TO220BV">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="A4982">
<packages>
<package name="ETSSOP24">
</package>
</packages>
<symbols>
<symbol name="A4982">
<pin name="CP2"/>
<pin name="VCP"/>
<pin name="VREG"/>
<pin name="MS1"/>
<pin name="MS2"/>
<pin name="ROSC"/>
<pin name="^RESET"/>
<pin name="^SLEEP"/>
<pin name="CP1"/>
<pin name="REF"/>
<pin name="DIR"/>
<pin name="STEP"/>
<pin name="^EN"/>
<pin name="OUT1A"/>
<pin name="SENSE1"/>
<pin name="OUT1B"/>
<pin name="OUT2A"/>
<pin name="SENSE2"/>
<pin name="OUT2B"/>
<pin name="VBB1"/>
<pin name="VDD"/>
<pin name="VBB2"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="PAD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="A4982">
<gates>
<gate name="G$1" symbol="A4982"/>
</gates>
<devices>
<device name="" package="ETSSOP24">
<connects>
<connect gate="G$1" pin="CP1" pad="P01"/>
<connect gate="G$1" pin="CP2" pad="P02"/>
<connect gate="G$1" pin="DIR" pad="P14"/>
<connect gate="G$1" pin="GND1" pad="P13"/>
<connect gate="G$1" pin="GND2" pad="P24"/>
<connect gate="G$1" pin="MS1" pad="P05"/>
<connect gate="G$1" pin="MS2" pad="P06"/>
<connect gate="G$1" pin="OUT1A" pad="P18"/>
<connect gate="G$1" pin="OUT1B" pad="P15"/>
<connect gate="G$1" pin="OUT2A" pad="P19"/>
<connect gate="G$1" pin="OUT2B" pad="P22"/>
<connect gate="G$1" pin="PAD" pad="EPAD"/>
<connect gate="G$1" pin="REF" pad="P12"/>
<connect gate="G$1" pin="ROSC" pad="P08"/>
<connect gate="G$1" pin="SENSE1" pad="P17"/>
<connect gate="G$1" pin="SENSE2" pad="P20"/>
<connect gate="G$1" pin="STEP" pad="P11"/>
<connect gate="G$1" pin="VBB1" pad="P16"/>
<connect gate="G$1" pin="VBB2" pad="P21"/>
<connect gate="G$1" pin="VCP" pad="P03"/>
<connect gate="G$1" pin="VDD" pad="P10"/>
<connect gate="G$1" pin="VREG" pad="P04"/>
<connect gate="G$1" pin="^EN" pad="P23"/>
<connect gate="G$1" pin="^RESET" pad="P07"/>
<connect gate="G$1" pin="^SLEEP" pad="P09"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Local Library">
<packages>
<package name="TACTILE-PTH-LED-12MM">
</package>
</packages>
<symbols>
<symbol name="SWITCH-MOMENTARY-LED">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SWITCH-MOMENTARY-LED" prefix="S">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-LED"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH-LED-12MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="ipc-7351-transistor">
<packages>
<package name="SOT95P280X135-3N">
</package>
<package name="SOT230P700X160-4N">
</package>
<package name="SOIC127P600X175-8AN">
</package>
</packages>
<symbols>
<symbol name="MOSFET-NCH">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MOSFET-NCH_" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-NCH"/>
</gates>
<devices>
<device name="SOT-23" package="SOT95P280X135-3N">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT-223" package="SOT230P700X160-4N">
<connects>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO-8" package="SOIC127P600X175-8AN">
<connects>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-amp">
<packages>
<package name="10X04MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;&lt;p&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_640456_W.pdf</description>
</package>
<package name="10X02MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;&lt;p&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_640456_W.pdf</description>
</package>
</packages>
<symbols>
<symbol name="MTA-1_4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="MTA-1_2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MTA04-100" prefix="J" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MTA-1_4"/>
</gates>
<devices>
<device name="" package="10X04MTA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MTA02-100" prefix="J" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MTA-1_2"/>
</gates>
<devices>
<device name="" package="10X02MTA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-weidmueller-sl35">
<packages>
<package name="180G-4">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
</package>
<package name="180G-2">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MALE-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="MALE-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="180G-4" prefix="X" uservalue="yes">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MALE-4"/>
</gates>
<devices>
<device name="" package="180G-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="180G-2" prefix="X" uservalue="yes">
<description>&lt;b&gt;WEIDMUELLER CLAMP CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MALE-2"/>
</gates>
<devices>
<device name="" package="180G-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Itead_BP_110825.lbr">
<packages>
<package name="HR911105A">
</package>
</packages>
<symbols>
<symbol name="HR911105A">
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="P4"/>
<pin name="RD-"/>
<pin name="GND"/>
<pin name="RD+"/>
<pin name="P5"/>
<pin name="NC"/>
<pin name="SHIELD0"/>
<pin name="SHIELD1"/>
<pin name="Y+"/>
<pin name="Y-"/>
<pin name="G+"/>
<pin name="G-"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HR911105A" prefix="RJ">
<description>SOC006</description>
<gates>
<gate name="G$1" symbol="HR911105A"/>
</gates>
<devices>
<device name="" package="HR911105A">
<connects>
<connect gate="G$1" pin="G+" pad="G+"/>
<connect gate="G$1" pin="G-" pad="G-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="RD+" pad="RD+"/>
<connect gate="G$1" pin="RD-" pad="RD-"/>
<connect gate="G$1" pin="SHIELD0" pad="SHIELD0"/>
<connect gate="G$1" pin="SHIELD1" pad="SHIELD1"/>
<connect gate="G$1" pin="TD+" pad="TD+"/>
<connect gate="G$1" pin="TD-" pad="TD-"/>
<connect gate="G$1" pin="Y+" pad="Y+"/>
<connect gate="G$1" pin="Y-" pad="Y-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
</packages>
<symbols>
<symbol name="78XX2GND">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="78L*" prefix="IC">
<description>&lt;b&gt;POSITOIV-VOLTAGE REGULATORS&lt;/b&gt;&lt;p&gt;
Output up to 100 mA&lt;b&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
<gates>
<gate name="G$1" symbol="78XX2GND"/>
</gates>
<devices>
<device name="F" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="2@1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="08"/>
<technology name="09"/>
<technology name="10"/>
<technology name="12"/>
<technology name="15"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="custom_esorensen">
<packages>
<package name="SOIC8">
</package>
</packages>
<symbols>
<symbol name="RAILS">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="BUFFER">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TC4427">
<gates>
<gate name="RAILS" symbol="RAILS"/>
<gate name="A" symbol="BUFFER"/>
<gate name="B" symbol="BUFFER"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="A" pin="P$1" pad="2"/>
<connect gate="A" pin="P$2" pad="7"/>
<connect gate="B" pin="P$1" pad="4"/>
<connect gate="B" pin="P$2" pad="5"/>
<connect gate="RAILS" pin="P$1" pad="6"/>
<connect gate="RAILS" pin="P$2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="AGND">
<pin name="AGND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AGND" prefix="AGND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VR1" symbol="AGND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SC74_INFINEON">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; Reflow soldering&lt;p&gt;
INFINEON, www.infineon.com/cmc_upload/0/000/010/257/eh_db_5b.pdf</description>
</package>
</packages>
<symbols>
<symbol name="P-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BSL207SP" prefix="Q">
<description>&lt;b&gt;OptiMOS(R)-P Small-Signal-Transistor&lt;/b&gt; P-Channel, Enhancement mode, Super Logic Level (2.5 V rated)&lt;p&gt;
Source: http://www.infineon.com/upload/Document/BSL207SP_Rev2.01.pdf</description>
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="" package="SC74_INFINEON">
<connects>
<connect gate="G$1" pin="D" pad="1 2 5 6"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="eric_sorensen">
<packages>
<package name="1715250000">
</package>
</packages>
<symbols>
<symbol name="JUMPER">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="5MMCONN">
<gates>
<gate name="G$1" symbol="JUMPER"/>
</gates>
<devices>
<device name="" package="1715250000">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="FRAME2" library="microbuilder" deviceset="FRAME_A3" device=""/>
<part name="IC1" library="microbuilder" deviceset="LPC1768" device="" value="LPC1769"/>
<part name="Q2" library="microbuilder" deviceset="CRYSTAL" device="THIN" value="12MHz"/>
<part name="C2" library="rcl" deviceset="C-EU" device="C0603" value="12pF"/>
<part name="C3" library="rcl" deviceset="C-EU" device="C0603" value="12pF"/>
<part name="SUPPLY1" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY2" library="supply2" deviceset="GND" device=""/>
<part name="P+1" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C8" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C9" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C10" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C11" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C12" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C13" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="P+2" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY3" library="supply2" deviceset="GND" device=""/>
<part name="C7" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="L1" library="SparkFun" deviceset="INDUCTOR" device="0603"/>
<part name="C6" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="R14" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+19" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY26" library="supply2" deviceset="GND" device=""/>
<part name="R8" library="resistor" deviceset="R-US_" device="R0603" value="33R"/>
<part name="R9" library="resistor" deviceset="R-US_" device="R0603" value="33R"/>
<part name="C4" library="rcl" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="C5" library="rcl" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="SUPPLY27" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY28" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY30" library="supply2" deviceset="GND" device=""/>
<part name="C1" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="P+21" library="SparkFun" deviceset="3.3V" device=""/>
<part name="VUSB" library="SparkFun" deviceset="5V" device="" value="VUSB"/>
<part name="R15" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+26" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY58" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY61" library="supply2" deviceset="GND" device=""/>
<part name="P+30" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R5" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R6" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="SUPPLY64" library="supply2" deviceset="GND" device=""/>
<part name="S1" library="SparkFun" deviceset="TAC_SWITCH" device="SMD"/>
<part name="LED1" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="LED2" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="LED3" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="LED4" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="R10" library="resistor" deviceset="R-US_" device="R0603" value="1k"/>
<part name="R11" library="resistor" deviceset="R-US_" device="R0603" value="1k"/>
<part name="R12" library="resistor" deviceset="R-US_" device="R0603" value="1k"/>
<part name="R13" library="resistor" deviceset="R-US_" device="R0603" value="1k"/>
<part name="SUPPLY65" library="supply2" deviceset="GND" device=""/>
<part name="JP5" library="SparkFun" deviceset="M06" device="POLAR"/>
<part name="S3" library="Local Library" deviceset="SWITCH-MOMENTARY-LED" device="PTH"/>
<part name="R16" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+28" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY20" library="supply2" deviceset="GND" device=""/>
<part name="R17" library="resistor" deviceset="R-US_" device="R0603" value="330R"/>
<part name="R3" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R2" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R1" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="JP26" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="JP14" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="JP16" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="JP19" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="JP21" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="JP22" library="SparkFun" deviceset="M03" device="POLAR"/>
<part name="P+4" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY21" library="supply2" deviceset="GND" device=""/>
<part name="P+8" library="SparkFun" deviceset="3.3V" device=""/>
<part name="JP8" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="S2" library="SparkFun" deviceset="TAC_SWITCH" device="SMD"/>
<part name="P+16" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C14" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="JP1" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="JP10" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="SUPPLY4" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY31" library="supply2" deviceset="GND" device=""/>
<part name="JP2" library="SparkFun" deviceset="M03" device="1X03_NO_SILK"/>
<part name="JP3" library="SparkFun" deviceset="M03" device="1X03_NO_SILK"/>
<part name="P+11" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY32" library="supply2" deviceset="GND" device=""/>
<part name="JP25" library="SparkFun" deviceset="M02" device="PTH"/>
<part name="JP24" library="SparkFun" deviceset="M02" device="PTH"/>
<part name="JP23" library="SparkFun" deviceset="M02" device="PTH"/>
<part name="FRAME3" library="microbuilder" deviceset="FRAME_A3" device=""/>
<part name="C21" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="C22" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="C23" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="P+5" library="SparkFun" deviceset="3.3V" device=""/>
<part name="P+12" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY39" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY40" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY41" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY42" library="supply2" deviceset="GND" device=""/>
<part name="C31" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="P+7" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R37" library="resistor" deviceset="R-US_" device="R0603" value="100K"/>
<part name="IC2" library="A4982" deviceset="A4982" device=""/>
<part name="C19" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C17" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY66" library="supply2" deviceset="GND" device=""/>
<part name="P+31" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C25" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY67" library="supply2" deviceset="GND" device=""/>
<part name="P+32" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY68" library="supply2" deviceset="GND" device=""/>
<part name="R26" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="C15" library="rcl" deviceset="C-EU" device="C0603" value=".22uF"/>
<part name="SUPPLY69" library="supply2" deviceset="GND" device=""/>
<part name="R24" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+33" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R31" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="R32" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="IC3" library="A4982" deviceset="A4982" device=""/>
<part name="C20" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C18" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY5" library="supply2" deviceset="GND" device=""/>
<part name="P+3" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C28" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY6" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY7" library="supply2" deviceset="GND" device=""/>
<part name="R27" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="C16" library="rcl" deviceset="C-EU" device="C0603" value=".22uF"/>
<part name="SUPPLY8" library="supply2" deviceset="GND" device=""/>
<part name="R28" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+6" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R33" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="R34" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="IC5" library="A4982" deviceset="A4982" device=""/>
<part name="C36" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C34" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY9" library="supply2" deviceset="GND" device=""/>
<part name="P+9" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C38" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY10" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY11" library="supply2" deviceset="GND" device=""/>
<part name="R40" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="C32" library="rcl" deviceset="C-EU" device="C0603" value=".22uF"/>
<part name="SUPPLY12" library="supply2" deviceset="GND" device=""/>
<part name="R41" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+13" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R46" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="R47" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="IC6" library="A4982" deviceset="A4982" device=""/>
<part name="C37" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C35" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY13" library="supply2" deviceset="GND" device=""/>
<part name="P+15" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C41" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY14" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY15" library="supply2" deviceset="GND" device=""/>
<part name="R43" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="C33" library="rcl" deviceset="C-EU" device="C0603" value=".22uF"/>
<part name="SUPPLY16" library="supply2" deviceset="GND" device=""/>
<part name="R44" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="P+34" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R48" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="R49" library="SparkFun" deviceset="RESISTOR" device="2512" value="0.05R"/>
<part name="C24" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="SL1" library="con-amp-quick" deviceset="M08" device=""/>
<part name="P+17" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R30" library="resistor" deviceset="R-US_" device="R0603" value="33K"/>
<part name="R22" library="resistor" deviceset="R-US_" device="R0603" value="NP"/>
<part name="R23" library="resistor" deviceset="R-US_" device="R0603" value="NP"/>
<part name="R38" library="resistor" deviceset="R-US_" device="R0603" value="NP"/>
<part name="R39" library="resistor" deviceset="R-US_" device="R0603" value="NP"/>
<part name="RN1" library="resistor-dil" deviceset="4R-N" device="0603-ARV" value="4.7K"/>
<part name="IC4" library="Geos" deviceset="MCP44X1" device=""/>
<part name="R35" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R36" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="J1" library="con-amp" deviceset="MTA04-100" device=""/>
<part name="J2" library="con-amp" deviceset="MTA04-100" device=""/>
<part name="J3" library="con-amp" deviceset="MTA04-100" device=""/>
<part name="J4" library="con-amp" deviceset="MTA04-100" device=""/>
<part name="X1" library="con-weidmueller-sl35" deviceset="180G-4" device=""/>
<part name="X2" library="con-weidmueller-sl35" deviceset="180G-4" device=""/>
<part name="X3" library="con-weidmueller-sl35" deviceset="180G-4" device=""/>
<part name="X4" library="con-weidmueller-sl35" deviceset="180G-4" device=""/>
<part name="C27" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C30" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C40" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C43" library="rcl" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="R25" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R29" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R42" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R45" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="FRAME4" library="microbuilder" deviceset="FRAME_A3" device=""/>
<part name="IC8" library="microbuilder" deviceset="LAN8720" device=""/>
<part name="R52" library="resistor" deviceset="R-US_" device="R0603" value="1.5K"/>
<part name="R64" library="resistor" deviceset="R-US_" device="R0603" value="1M"/>
<part name="R63" library="resistor" deviceset="R-US_" device="R0603" value="12.1K"/>
<part name="Q3" library="microbuilder" deviceset="CRYSTAL" device="THIN" value="25MHz"/>
<part name="C58" library="resistor" deviceset="C-EU" device="C0603" value="12pF"/>
<part name="C59" library="resistor" deviceset="C-EU" device="C0603" value="12pF"/>
<part name="SUPPLY44" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY45" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY43" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY46" library="supply2" deviceset="GND" device=""/>
<part name="R50" library="resistor" deviceset="R-US_" device="R0603" value="330R"/>
<part name="R62" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R61" library="resistor" deviceset="R-US_" device="R0603" value="330R"/>
<part name="SUPPLY47" library="supply2" deviceset="GND" device=""/>
<part name="P+10" library="SparkFun" deviceset="3.3V" device=""/>
<part name="FB1" library="microbuilder" deviceset="FERRITE" device=""/>
<part name="C45" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="C46" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C47" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY48" library="supply2" deviceset="GND" device=""/>
<part name="P+14" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C50" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="C51" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY49" library="supply2" deviceset="GND" device=""/>
<part name="C48" library="SparkFun" deviceset="CAP_POL" device="1206" value="1uF"/>
<part name="C49" library="resistor" deviceset="C-EU" device="C0603K" value="470pF"/>
<part name="C53" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C52" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C54" library="resistor" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="C55" library="resistor" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="C56" library="resistor" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="C57" library="resistor" deviceset="C-EU" device="C0603" value="18pF"/>
<part name="SUPPLY50" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY51" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY52" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY53" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY54" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY55" library="supply2" deviceset="GND" device=""/>
<part name="IC7" library="microbuilder" deviceset="74LVC1G04" device=""/>
<part name="R51" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="SUPPLY56" library="supply2" deviceset="GND" device=""/>
<part name="C44" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY57" library="supply2" deviceset="GND" device=""/>
<part name="P+18" library="SparkFun" deviceset="3.3V" device=""/>
<part name="IC10" library="SparkFun" deviceset="V_REG_LM1117" device="SOT223" value="LM1117-3.3V"/>
<part name="VUSB2" library="SparkFun" deviceset="5V" device="" value="VUSB"/>
<part name="P+27" library="SparkFun" deviceset="3.3V" device=""/>
<part name="C65" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="C64" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="SUPPLY59" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY60" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY63" library="supply2" deviceset="GND" device=""/>
<part name="D2" library="microbuilder" deviceset="DIODE" device="SMA" value="MBRA210LT3"/>
<part name="LED9" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="R77" library="resistor" deviceset="R-US_" device="R0603" value="1k"/>
<part name="Q6" library="transistor-power" deviceset="IRF540" device="" value="AOT240L"/>
<part name="Q7" library="transistor-power" deviceset="IRF540" device="" value="AOT240L"/>
<part name="SUPPLY18" library="supply2" deviceset="GND" device=""/>
<part name="R73" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="R75" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="R69" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="R70" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="SUPPLY22" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY23" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY24" library="supply2" deviceset="GND" device=""/>
<part name="C60" library="SparkFun" deviceset="CAP_POL" device="E" value="100uF"/>
<part name="POWER" library="Geos" deviceset="HDD-ATX_CON" device="" value="POWER"/>
<part name="SUPPLY35" library="supply2" deviceset="GND" device=""/>
<part name="R78" library="resistor" deviceset="R-US_" device="R0603" value="2.2K"/>
<part name="LED10" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="Q8" library="ipc-7351-transistor" deviceset="MOSFET-NCH_" device="SOT-223" value="ZXMN4A06GTA"/>
<part name="Q9" library="ipc-7351-transistor" deviceset="MOSFET-NCH_" device="SOT-223" value="ZXMN4A06GTA"/>
<part name="R74" library="resistor" deviceset="R-US_" device="R0603" value="10k"/>
<part name="R76" library="resistor" deviceset="R-US_" device="R0603" value="10k"/>
<part name="R71" library="resistor" deviceset="R-US_" device="R0603" value="10k"/>
<part name="R72" library="resistor" deviceset="R-US_" device="R0603" value="10k"/>
<part name="C61" library="SparkFun" deviceset="CAP_POL" device="1206" value="10uF"/>
<part name="D1" library="microbuilder" deviceset="DIODE" device="SMA" value="MBRA210LT3"/>
<part name="C63" library="SparkFun" deviceset="CAP_POL" device="D" value="100uF"/>
<part name="J10" library="SparkFun" deviceset="POWER_JACK" device="SMD"/>
<part name="X12" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="X11" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="X7" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="X8" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="X10" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="X6" library="con-weidmueller-sl35" deviceset="180G-2" device=""/>
<part name="U$1" library="Geos" deviceset="ETH1506S" device=""/>
<part name="JP28" library="jumper" deviceset="JP1E" device=""/>
<part name="JP11" library="jumper" deviceset="JP1E" device=""/>
<part name="JP27" library="jumper" deviceset="JP1E" device=""/>
<part name="J8" library="con-amp" deviceset="MTA02-100" device=""/>
<part name="J6" library="con-amp" deviceset="MTA02-100" device=""/>
<part name="J9" library="con-amp" deviceset="MTA02-100" device=""/>
<part name="JP17" library="SparkFun" deviceset="M03" device="PTH"/>
<part name="JP18" library="SparkFun" deviceset="M03" device="PTH"/>
<part name="SUPPLY37" library="supply2" deviceset="GND" device=""/>
<part name="P+20" library="SparkFun" deviceset="3.3V" device=""/>
<part name="R65" library="resistor" deviceset="R-US_" device="R0603" value="5.6K"/>
<part name="LED5" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="R66" library="resistor" deviceset="R-US_" device="R0603" value="5.6K"/>
<part name="R67" library="resistor" deviceset="R-US_" device="R0603" value="5.6K"/>
<part name="R68" library="resistor" deviceset="R-US_" device="R0603" value="5.6K"/>
<part name="LED6" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="LED7" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="LED8" library="led" deviceset="LED" device="CHIP-LED0805"/>
<part name="C26" library="SparkFun" deviceset="CAP_POL" device="E" value="100uF"/>
<part name="C29" library="SparkFun" deviceset="CAP_POL" device="E" value="100uF"/>
<part name="C39" library="SparkFun" deviceset="CAP_POL" device="E" value="100uF"/>
<part name="C42" library="SparkFun" deviceset="CAP_POL" device="E" value="100uF"/>
<part name="U1" library="SparkFun" deviceset="USD-SOCKET" device="NEW"/>
<part name="R7" library="resistor" deviceset="R-US_" device="R0603" value="1.5K"/>
<part name="P+22" library="SparkFun" deviceset="3.3V" device=""/>
<part name="JP4" library="SparkFun" deviceset="M03" device="1X03_NO_SILK"/>
<part name="JP6" library="SparkFun" deviceset="M03" device="1X03_NO_SILK"/>
<part name="P+29" library="SparkFun" deviceset="3.3V" device=""/>
<part name="SUPPLY36" library="supply2" deviceset="GND" device=""/>
<part name="R53" library="resistor" deviceset="R-US_" device="R0603" value="10K"/>
<part name="R58" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="R59" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="R60" library="resistor" deviceset="R-US_" device="R0603" value="22R"/>
<part name="RJ1" library="Itead_BP_110825.lbr" deviceset="HR911105A" device=""/>
<part name="SUPPLY19" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY62" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY70" library="supply2" deviceset="GND" device=""/>
<part name="R54" library="resistor" deviceset="R-US_" device="R0603" value="49.9R"/>
<part name="R55" library="resistor" deviceset="R-US_" device="R0603" value="49.9R"/>
<part name="R56" library="resistor" deviceset="R-US_" device="R0603" value="49.9R"/>
<part name="R57" library="resistor" deviceset="R-US_" device="R0603" value="49.9R"/>
<part name="JP20" library="SparkFun" deviceset="M03" device="PTH"/>
<part name="JP13" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="SUPPLY71" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY72" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY73" library="supply2" deviceset="GND" device=""/>
<part name="C62" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="SUPPLY74" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY75" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY76" library="supply2" deviceset="GND" device=""/>
<part name="SUPPLY77" library="supply2" deviceset="GND" device=""/>
<part name="JP7" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="JP9" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="JP12" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="JP15" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="JP29" library="SparkFun" deviceset="M04" device="1X04_NO_SILK"/>
<part name="SUPPLY78" library="supply2" deviceset="GND" device=""/>
<part name="C66" library="resistor" deviceset="C-EU" device="C0603" value=".1uF"/>
<part name="JP30" library="SparkFun" deviceset="JUMPER-2" device="SMD-NC"/>
<part name="JP31" library="SparkFun" deviceset="JUMPER-2" device="SMD-NC"/>
<part name="U$2" library="custom_esorensen" deviceset="TC4427" device=""/>
<part name="AGND1" library="supply1" deviceset="AGND" device=""/>
<part name="AGND2" library="supply1" deviceset="AGND" device=""/>
<part name="AGND3" library="supply1" deviceset="AGND" device=""/>
<part name="C67" library="resistor" deviceset="C-EU" device="C0805" value="1uF"/>
<part name="IC11" library="linear" deviceset="78L*" device="F" technology="12"/>
<part name="X14" library="SparkFun" deviceset="USB" device="PTH"/>
<part name="SJ1" library="SparkFun" deviceset="SOLDERJUMPER_2WAY" device="S"/>
<part name="P+23" library="SparkFun" deviceset="3.3V" device=""/>
<part name="Q1" library="transistor-fet" deviceset="BSL207SP" device=""/>
<part name="U$3" library="SparkFun" deviceset="5V" device=""/>
<part name="U$4" library="SparkFun" deviceset="5V" device=""/>
<part name="U$5" library="eric_sorensen" deviceset="5MMCONN" device=""/>
<part name="U$6" library="eric_sorensen" deviceset="5MMCONN" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>SD Card connector</text>
<text>UART0</text>
<text>(Also for ISP Loading)</text>
<text>http://smoothieware.org</text>
<text>Symbol reversed in Sparkfun</text>
<text>Smoothieboard</text>
<text>by: Arthur Wolf</text>
<text>produced by: Trinity Labs</text>
<text>Licensed under GPL: http://www.gnu.org/licenses/gpl.html</text>
<text>Thanks for the support and contributions of the Reprap Community</text>
</plain>
<busses>
</busses>
<nets>
<net name="N$1">
<segment>
<pinref part="IC1" gate="G$1" pin="XTAL1"/>
<pinref part="Q2" gate="G$1" pin="2"/>
<pinref part="C2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="Q2" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="XTAL2"/>
<pinref part="C3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="SUPPLY1" gate="GND" pin="GND"/>
<pinref part="C2" gate="G$1" pin="2"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY2" gate="GND" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="VSS1"/>
<pinref part="IC1" gate="G$1" pin="VSS2"/>
<pinref part="IC1" gate="G$1" pin="VSS3"/>
<pinref part="IC1" gate="G$1" pin="VSS4"/>
<pinref part="IC1" gate="G$1" pin="VSS5"/>
<pinref part="IC1" gate="G$1" pin="VSS6"/>
</segment>
<segment>
<pinref part="C8" gate="G$1" pin="1"/>
<pinref part="C13" gate="G$1" pin="1"/>
<pinref part="C12" gate="G$1" pin="1"/>
<pinref part="C11" gate="G$1" pin="1"/>
<pinref part="C10" gate="G$1" pin="1"/>
<pinref part="C9" gate="G$1" pin="1"/>
<pinref part="SUPPLY3" gate="GND" pin="GND"/>
<pinref part="C7" gate="G$1" pin="-"/>
<pinref part="C14" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY26" gate="GND" pin="GND"/>
<pinref part="S1" gate="S" pin="3"/>
<pinref part="S1" gate="S" pin="4"/>
</segment>
<segment>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="C5" gate="G$1" pin="1"/>
<pinref part="SUPPLY27" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY28" gate="GND" pin="GND"/>
<pinref part="X14" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY30" gate="GND" pin="GND"/>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="U1" gate="G$1" pin="SHIELD@3"/>
<pinref part="U1" gate="G$1" pin="SHIELD@4"/>
<pinref part="C67" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY65" gate="GND" pin="GND"/>
<pinref part="LED1" gate="G$1" pin="C"/>
<pinref part="LED2" gate="G$1" pin="C"/>
<pinref part="LED3" gate="G$1" pin="C"/>
<pinref part="LED4" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="JP5" gate="G$1" pin="1"/>
<pinref part="SUPPLY61" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY20" gate="GND" pin="GND"/>
<pinref part="S3" gate="G$1" pin="2"/>
<pinref part="JP23" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY21" gate="GND" pin="GND"/>
<pinref part="JP22" gate="G$1" pin="2"/>
<pinref part="JP21" gate="G$1" pin="2"/>
<pinref part="JP19" gate="G$1" pin="2"/>
<pinref part="JP16" gate="G$1" pin="2"/>
<pinref part="JP14" gate="G$1" pin="2"/>
<pinref part="JP26" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY58" gate="GND" pin="GND"/>
<pinref part="S2" gate="S" pin="4"/>
<pinref part="S2" gate="S" pin="3"/>
</segment>
<segment>
<pinref part="JP10" gate="G$1" pin="4"/>
<pinref part="JP10" gate="G$1" pin="1"/>
<pinref part="JP10" gate="G$1" pin="2"/>
<pinref part="JP10" gate="G$1" pin="3"/>
<pinref part="SUPPLY4" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY31" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="JP3" gate="G$1" pin="3"/>
<pinref part="SUPPLY32" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY37" gate="GND" pin="GND"/>
<pinref part="JP17" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="JP6" gate="G$1" pin="3"/>
<pinref part="SUPPLY36" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY77" gate="GND" pin="GND"/>
<pinref part="JP7" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="SUPPLY76" gate="GND" pin="GND"/>
<pinref part="JP9" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="SUPPLY75" gate="GND" pin="GND"/>
<pinref part="JP12" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="SUPPLY74" gate="GND" pin="GND"/>
<pinref part="JP15" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="2"/>
<pinref part="SUPPLY64" gate="GND" pin="GND"/>
</segment>
</net>
<net name="3.3V">
<segment>
<pinref part="P+1" gate="G$1" pin="3.3V"/>
<pinref part="IC1" gate="G$1" pin="VDD(3V3)4"/>
<pinref part="IC1" gate="G$1" pin="VDD(3V3)3"/>
<pinref part="IC1" gate="G$1" pin="VDD(3V3)2"/>
<pinref part="IC1" gate="G$1" pin="VDD(3V3)1"/>
<pinref part="IC1" gate="G$1" pin="VDD(REG)(3V3)2"/>
<pinref part="IC1" gate="G$1" pin="VDD(REG)(3V3)1"/>
</segment>
<segment>
<pinref part="C8" gate="G$1" pin="2"/>
<pinref part="C13" gate="G$1" pin="2"/>
<pinref part="C10" gate="G$1" pin="2"/>
<pinref part="C9" gate="G$1" pin="2"/>
<pinref part="C11" gate="G$1" pin="2"/>
<pinref part="C12" gate="G$1" pin="2"/>
<pinref part="P+2" gate="G$1" pin="3.3V"/>
<pinref part="C7" gate="G$1" pin="+"/>
<pinref part="L1" gate="G$1" pin="2"/>
<pinref part="C14" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+19" gate="G$1" pin="3.3V"/>
<pinref part="R14" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+26" gate="G$1" pin="3.3V"/>
<pinref part="R15" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
<pinref part="P+30" gate="G$1" pin="3.3V"/>
<pinref part="R6" gate="G$1" pin="2"/>
<pinref part="Q1" gate="G$1" pin="S"/>
</segment>
<segment>
<pinref part="R16" gate="G$1" pin="2"/>
<pinref part="P+28" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="P+21" gate="G$1" pin="3.3V"/>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="C1" gate="G$1" pin="2"/>
<pinref part="U1" gate="G$1" pin="VCC"/>
<pinref part="C67" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+4" gate="G$1" pin="3.3V"/>
<pinref part="JP22" gate="G$1" pin="1"/>
<pinref part="JP21" gate="G$1" pin="1"/>
<pinref part="JP19" gate="G$1" pin="1"/>
<pinref part="JP16" gate="G$1" pin="1"/>
<pinref part="JP14" gate="G$1" pin="1"/>
<pinref part="JP26" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+8" gate="G$1" pin="3.3V"/>
<pinref part="JP1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+16" gate="G$1" pin="3.3V"/>
<pinref part="IC1" gate="G$1" pin="VBAT"/>
</segment>
<segment>
<pinref part="JP2" gate="G$1" pin="1"/>
<pinref part="P+11" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="JP17" gate="G$1" pin="2"/>
<pinref part="P+20" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="R17" gate="G$1" pin="1"/>
<pinref part="P+22" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="JP4" gate="G$1" pin="1"/>
<pinref part="P+29" gate="G$1" pin="3.3V"/>
</segment>
<segment>
<pinref part="P+23" gate="G$1" pin="3.3V"/>
<pinref part="SJ1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="AVCC">
<segment>
<pinref part="IC1" gate="G$1" pin="VDDA"/>
<pinref part="L1" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="VREFP"/>
<pinref part="C6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RESET">
<segment>
<pinref part="IC1" gate="G$1" pin="RESET"/>
</segment>
<segment>
<pinref part="R14" gate="G$1" pin="1"/>
<pinref part="S1" gate="S" pin="1"/>
<pinref part="S1" gate="S" pin="2"/>
</segment>
<segment>
<pinref part="JP25" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ENET_TXD0">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[0]/ENET_TXD0"/>
</segment>
</net>
<net name="ENET_TXD1">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[1]/ENET_TXD1"/>
</segment>
</net>
<net name="ENET_TX_EN">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[4]/ENET_TX_EN"/>
</segment>
</net>
<net name="ENET_CRS">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[8]/ENET_CRS"/>
</segment>
</net>
<net name="ENET_RXD0">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[9]/ENET_RXD0"/>
</segment>
</net>
<net name="ENET_RXD1">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[10]/ENET_RXD1"/>
</segment>
</net>
<net name="ENET_RX_ER">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[14]/ENET_RX_ER"/>
</segment>
</net>
<net name="ENET_REF_CLK">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[15]/ENET_REF_CLK"/>
</segment>
</net>
<net name="ENET_MDC">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[16]/ENET_MDC"/>
</segment>
</net>
<net name="ENET_MDIO">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[17]/ENET_MDIO"/>
</segment>
</net>
<net name="USB_D-">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[30]/USB_D-"/>
<pinref part="R9" gate="G$1" pin="2"/>
<pinref part="C4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="USB_D+">
<segment>
<pinref part="R8" gate="G$1" pin="2"/>
<pinref part="IC1" gate="G$1" pin="P0[29]/USB_D+"/>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$61">
<segment>
<pinref part="R8" gate="G$1" pin="1"/>
<pinref part="X14" gate="G$1" pin="D+"/>
</segment>
</net>
<net name="N$62">
<segment>
<pinref part="R9" gate="G$1" pin="1"/>
<pinref part="X14" gate="G$1" pin="D-"/>
</segment>
</net>
<net name="SD_MOSI">
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="U1" gate="G$1" pin="DI"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
</segment>
<segment>
<pinref part="JP6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SD_MISO">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="U1" gate="G$1" pin="DO"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
</segment>
<segment>
<pinref part="JP6" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SD_SCK">
<segment>
<pinref part="U1" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
</segment>
<segment>
<pinref part="JP4" gate="G$1" pin="3"/>
</segment>
</net>
<net name="SD_CS">
<segment>
<pinref part="U1" gate="G$1" pin="CS"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
</segment>
<segment>
<pinref part="JP4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SD_IRQ">
<segment>
<pinref part="IC1" gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]"/>
</segment>
<segment>
<pinref part="JP20" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SD_CD">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[11]/EINT1/I2STX_CLK"/>
</segment>
<segment>
<pinref part="JP20" gate="G$1" pin="3"/>
</segment>
</net>
<net name="SD_WP">
<segment>
<pinref part="IC1" gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
</segment>
<segment>
<pinref part="JP20" gate="G$1" pin="2"/>
</segment>
</net>
<net name="EN1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
</segment>
<segment>
<pinref part="JP7" gate="G$1" pin="1"/>
</segment>
</net>
<net name="DIR1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
</segment>
<segment>
<pinref part="JP7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="STP1">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[0]/PWM1[1]/TXD1"/>
</segment>
<segment>
<pinref part="JP7" gate="G$1" pin="3"/>
</segment>
</net>
<net name="STP2">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[1]/PWM1[2]/RXD1"/>
</segment>
<segment>
<pinref part="JP9" gate="G$1" pin="3"/>
</segment>
</net>
<net name="STP3">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
</segment>
<segment>
<pinref part="JP12" gate="G$1" pin="3"/>
</segment>
</net>
<net name="EN4">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[21]/RI1/RD1"/>
</segment>
<segment>
<pinref part="JP15" gate="G$1" pin="1"/>
</segment>
</net>
<net name="JTAG-TRST">
<segment>
<pinref part="IC1" gate="G$1" pin="TRST"/>
</segment>
</net>
<net name="JTAG-TDI">
<segment>
<pinref part="IC1" gate="G$1" pin="TDI"/>
</segment>
</net>
<net name="JTAG-TMS">
<segment>
<pinref part="IC1" gate="G$1" pin="TMS/SWDIO"/>
</segment>
</net>
<net name="JTAG-TCK">
<segment>
<pinref part="IC1" gate="G$1" pin="TCK/SWDCLK"/>
</segment>
</net>
<net name="JTAG-RTCK">
<segment>
<pinref part="IC1" gate="G$1" pin="RTCK"/>
</segment>
</net>
<net name="JTAG-TDO">
<segment>
<pinref part="IC1" gate="G$1" pin="TDO/SWO"/>
</segment>
</net>
<net name="DIR4">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[22]/RTS1/TD1"/>
</segment>
<segment>
<pinref part="JP15" gate="G$1" pin="2"/>
</segment>
</net>
<net name="STP4">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
</segment>
<segment>
<pinref part="JP15" gate="G$1" pin="3"/>
</segment>
</net>
<net name="TH1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
</segment>
</net>
<net name="TH2">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
</segment>
</net>
<net name="TH3">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
</segment>
</net>
<net name="RX_0">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[3]/RXD0/AD0[6]"/>
</segment>
<segment>
<pinref part="JP5" gate="G$1" pin="4"/>
</segment>
</net>
<net name="TX_0">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[2]/TXD0/AD0[7]"/>
</segment>
<segment>
<pinref part="JP5" gate="G$1" pin="5"/>
</segment>
</net>
<net name="VUSB">
<segment>
<pinref part="VUSB" gate="G$1" pin="5V"/>
<pinref part="X14" gate="G$1" pin="VBUS"/>
</segment>
</net>
<net name="RSTOUT">
<segment>
<pinref part="IC1" gate="G$1" pin="RSTOUT"/>
</segment>
</net>
<net name="ISP_BOOT">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[10]/EINT0/NMI"/>
</segment>
<segment>
<pinref part="R15" gate="G$1" pin="1"/>
<pinref part="S2" gate="S" pin="2"/>
<pinref part="S2" gate="S" pin="1"/>
</segment>
<segment>
<pinref part="JP25" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[28]/SCL0/USB_SCL"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="4"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="IC1" gate="G$1" pin="P0[27]/SDA0/USB_SDA"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$84">
<segment>
<pinref part="LED4" gate="G$1" pin="A"/>
<pinref part="R13" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$85">
<segment>
<pinref part="LED3" gate="G$1" pin="A"/>
<pinref part="R12" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$86">
<segment>
<pinref part="LED2" gate="G$1" pin="A"/>
<pinref part="R11" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$87">
<segment>
<pinref part="LED1" gate="G$1" pin="A"/>
<pinref part="R10" gate="G$1" pin="1"/>
</segment>
</net>
<net name="LED1">
<segment>
<pinref part="R10" gate="G$1" pin="2"/>
<pinref part="JP29" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
</segment>
</net>
<net name="LED2">
<segment>
<pinref part="R11" gate="G$1" pin="2"/>
<pinref part="JP29" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P1[19]/MC0A/USB_PPWR/CAP1[1]"/>
</segment>
</net>
<net name="LED3">
<segment>
<pinref part="R12" gate="G$1" pin="2"/>
<pinref part="JP29" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P1[20]/MCFB0/PWM1[2]/SCK0"/>
</segment>
</net>
<net name="LED4">
<segment>
<pinref part="R13" gate="G$1" pin="2"/>
<pinref part="JP29" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
</segment>
</net>
<net name="TH4">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3"/>
</segment>
</net>
<net name="RTS">
<segment>
<pinref part="JP5" gate="G$1" pin="6"/>
</segment>
</net>
<net name="CTS">
<segment>
<pinref part="JP5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="P2.6">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
</segment>
<segment>
<pinref part="JP13" gate="G$1" pin="1"/>
</segment>
</net>
<net name="P2.7">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[7]/RD2/RTS1"/>
</segment>
<segment>
<pinref part="JP13" gate="G$1" pin="4"/>
</segment>
</net>
<net name="P2.8">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[8]/TD2/TXD2"/>
</segment>
<segment>
<pinref part="JP18" gate="G$1" pin="1"/>
</segment>
</net>
<net name="P2.9">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[9]/USB_CONNECT/RXD2"/>
</segment>
<segment>
<pinref part="Q1" gate="G$1" pin="G"/>
</segment>
</net>
<net name="P2.13">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[13]/EINT3/I2STX_SDA"/>
</segment>
<segment>
<pinref part="JP18" gate="G$1" pin="3"/>
</segment>
</net>
<net name="P4.29">
<segment>
<pinref part="IC1" gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
</segment>
<segment>
<pinref part="JP18" gate="G$1" pin="2"/>
</segment>
</net>
<net name="X_MAX">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[25]/MC1A/MAT1[1]"/>
</segment>
<segment>
<pinref part="JP14" gate="G$1" pin="3"/>
</segment>
</net>
<net name="X_MIN">
<segment>
<pinref part="JP26" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P1[24]/MCFB2/PWM1[5]/MOSI0"/>
</segment>
</net>
<net name="PLAY">
<segment>
<pinref part="R16" gate="G$1" pin="1"/>
<pinref part="S3" gate="G$1" pin="1"/>
<pinref part="JP23" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="P2[12]/EINT2/I2STX_WS"/>
</segment>
</net>
<net name="N$73">
<segment>
<pinref part="R17" gate="G$1" pin="2"/>
<pinref part="JP24" gate="G$1" pin="1"/>
<pinref part="S3" gate="G$1" pin="C"/>
</segment>
</net>
<net name="PLAY_LED">
<segment>
<pinref part="IC1" gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
</segment>
<segment>
<pinref part="JP24" gate="G$1" pin="2"/>
<pinref part="S3" gate="G$1" pin="A"/>
</segment>
</net>
<net name="EN2">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]"/>
</segment>
<segment>
<pinref part="JP9" gate="G$1" pin="1"/>
</segment>
</net>
<net name="DIR2">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]"/>
</segment>
<segment>
<pinref part="JP9" gate="G$1" pin="2"/>
</segment>
</net>
<net name="EN3">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[19]/DSR1/SDA1"/>
</segment>
<segment>
<pinref part="JP12" gate="G$1" pin="1"/>
</segment>
</net>
<net name="DIR3">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[20]/DTR1/SCL1"/>
</segment>
<segment>
<pinref part="JP12" gate="G$1" pin="2"/>
</segment>
</net>
<net name="Y_MAX">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
</segment>
<segment>
<pinref part="JP19" gate="G$1" pin="3"/>
</segment>
</net>
<net name="Z_MIN">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[28]/MC2A/PCAP1[0]/MAT0[0]"/>
</segment>
<segment>
<pinref part="JP21" gate="G$1" pin="3"/>
</segment>
</net>
<net name="Z_MAX">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[29]/MC2B/PCAP1[1]/MAT0[1]"/>
</segment>
<segment>
<pinref part="JP22" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PWM0">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
</segment>
<segment>
<pinref part="JP13" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PWM1">
<segment>
<pinref part="IC1" gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
</segment>
<segment>
<pinref part="JP13" gate="G$1" pin="3"/>
</segment>
</net>
<net name="Y_MIN">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[26]/MC1B/PWM1[6]/CAP0[0]"/>
</segment>
<segment>
<pinref part="JP16" gate="G$1" pin="3"/>
</segment>
</net>
<net name="POT_SCL">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[1]/TD1/RXD3/SCL1"/>
</segment>
</net>
<net name="POT_SDA">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[0]/RD1/TXD3/SDA1"/>
</segment>
</net>
<net name="P1_22">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[22]/MC0B/USB_PWRD/MAT1[0]"/>
</segment>
<segment>
<pinref part="JP8" gate="G$1" pin="1"/>
</segment>
</net>
<net name="P1_23">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[23]/MCFB1/PWM1[4]/MISO0"/>
</segment>
<segment>
<pinref part="JP8" gate="G$1" pin="2"/>
</segment>
</net>
<net name="P1_30">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[30]/VBUS/AD0[4]"/>
</segment>
<segment>
<pinref part="JP8" gate="G$1" pin="4"/>
</segment>
</net>
<net name="P1_31">
<segment>
<pinref part="IC1" gate="G$1" pin="P1[31]/SCK1/AD0[5]"/>
</segment>
<segment>
<pinref part="JP8" gate="G$1" pin="3"/>
</segment>
</net>
<net name="SSEL1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL"/>
</segment>
<segment>
<pinref part="JP2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SCK1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[15]/TXD1/SCK0/SCK"/>
</segment>
<segment>
<pinref part="JP2" gate="G$1" pin="3"/>
</segment>
</net>
<net name="MISO1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[17]/CTS1/MISO0/MISO"/>
</segment>
<segment>
<pinref part="JP3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="MOSI1">
<segment>
<pinref part="IC1" gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI"/>
</segment>
<segment>
<pinref part="JP3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VBB">
<segment>
<pinref part="JP17" gate="G$1" pin="1"/>
</segment>
</net>
<net name="5V">
<segment>
<pinref part="U$4" gate="G$1" pin="5V"/>
<pinref part="SJ1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$51">
<segment>
<pinref part="R7" gate="G$1" pin="2"/>
<pinref part="Q1" gate="G$1" pin="D"/>
</segment>
</net>
<net name="AGND">
<segment>
<pinref part="IC1" gate="G$1" pin="VREFN"/>
<pinref part="IC1" gate="G$1" pin="VSSA"/>
<pinref part="AGND1" gate="VR1" pin="AGND"/>
</segment>
<segment>
<pinref part="C6" gate="G$1" pin="2"/>
<pinref part="AGND2" gate="VR1" pin="AGND"/>
</segment>
</net>
<net name="N$23">
<segment>
<pinref part="JP5" gate="G$1" pin="3"/>
<pinref part="SJ1" gate="G$1" pin="2"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
<text>SW002:</text>
<text>MS1</text>
<text>MS2</text>
<text>L</text>
<text>L</text>
<text>L</text>
<text>L</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>H</text>
<text>FULL</text>
<text>HALF</text>
<text>4th</text>
<text>16 th</text>
<text>Thermistor Connection</text>
<text>http://smoothieware.org</text>
</plain>
<busses>
</busses>
<nets>
<net name="EN1">
<segment>
<pinref part="IC2" gate="G$1" pin="^EN"/>
</segment>
</net>
<net name="DIR1">
<segment>
<pinref part="IC2" gate="G$1" pin="DIR"/>
</segment>
</net>
<net name="VBB">
<segment>
<pinref part="IC2" gate="G$1" pin="VBB1"/>
<pinref part="IC2" gate="G$1" pin="VBB2"/>
<pinref part="C27" gate="G$1" pin="1"/>
<pinref part="C26" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="C17" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="VBB1"/>
<pinref part="IC3" gate="G$1" pin="VBB2"/>
<pinref part="C30" gate="G$1" pin="1"/>
<pinref part="C29" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="C18" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="VBB1"/>
<pinref part="IC5" gate="G$1" pin="VBB2"/>
<pinref part="C40" gate="G$1" pin="1"/>
<pinref part="C39" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="C34" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="VBB1"/>
<pinref part="IC6" gate="G$1" pin="VBB2"/>
<pinref part="C43" gate="G$1" pin="1"/>
<pinref part="C42" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="C35" gate="G$1" pin="1"/>
</segment>
</net>
<net name="3.3V">
<segment>
<pinref part="P+5" gate="G$1" pin="3.3V"/>
<pinref part="R35" gate="G$1" pin="2"/>
<pinref part="R36" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+12" gate="G$1" pin="3.3V"/>
<pinref part="R37" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+7" gate="G$1" pin="3.3V"/>
<pinref part="C31" gate="G$1" pin="2"/>
<pinref part="IC4" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="C25" gate="G$1" pin="1"/>
<pinref part="P+31" gate="G$1" pin="3.3V"/>
<pinref part="IC2" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="P+32" gate="G$1" pin="3.3V"/>
<pinref part="JP30" gate="A" pin="2"/>
<pinref part="JP31" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="R24" gate="G$1" pin="2"/>
<pinref part="P+33" gate="G$1" pin="3.3V"/>
<pinref part="R22" gate="G$1" pin="1"/>
<pinref part="R25" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C28" gate="G$1" pin="1"/>
<pinref part="P+3" gate="G$1" pin="3.3V"/>
<pinref part="IC3" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="R28" gate="G$1" pin="2"/>
<pinref part="P+6" gate="G$1" pin="3.3V"/>
<pinref part="R23" gate="G$1" pin="2"/>
<pinref part="R29" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C38" gate="G$1" pin="1"/>
<pinref part="P+9" gate="G$1" pin="3.3V"/>
<pinref part="IC5" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="R41" gate="G$1" pin="2"/>
<pinref part="P+13" gate="G$1" pin="3.3V"/>
<pinref part="R38" gate="G$1" pin="2"/>
<pinref part="R42" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C41" gate="G$1" pin="1"/>
<pinref part="P+15" gate="G$1" pin="3.3V"/>
<pinref part="IC6" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="R44" gate="G$1" pin="2"/>
<pinref part="P+34" gate="G$1" pin="3.3V"/>
<pinref part="R39" gate="G$1" pin="2"/>
<pinref part="R45" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+17" gate="G$1" pin="3.3V"/>
<pinref part="R30" gate="G$1" pin="2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="SUPPLY39" gate="GND" pin="GND"/>
<pinref part="IC4" gate="G$1" pin="P3B"/>
<pinref part="IC4" gate="G$1" pin="HVC/A0"/>
</segment>
<segment>
<pinref part="SUPPLY40" gate="GND" pin="GND"/>
<pinref part="IC4" gate="G$1" pin="VSS"/>
<pinref part="IC4" gate="G$1" pin="P1B"/>
</segment>
<segment>
<pinref part="SUPPLY41" gate="GND" pin="GND"/>
<pinref part="IC4" gate="G$1" pin="P0B"/>
<pinref part="IC4" gate="G$1" pin="A1"/>
</segment>
<segment>
<pinref part="SUPPLY42" gate="GND" pin="GND"/>
<pinref part="C31" gate="G$1" pin="1"/>
<pinref part="IC4" gate="G$1" pin="P2B"/>
</segment>
<segment>
<pinref part="SUPPLY66" gate="GND" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="GND1"/>
<pinref part="IC2" gate="G$1" pin="PAD"/>
<pinref part="IC2" gate="G$1" pin="GND2"/>
<pinref part="C25" gate="G$1" pin="2"/>
<pinref part="C27" gate="G$1" pin="2"/>
<pinref part="C26" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="SUPPLY67" gate="GND" pin="GND"/>
<pinref part="R31" gate="G$1" pin="1"/>
<pinref part="R32" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY68" gate="GND" pin="GND"/>
<pinref part="R26" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C15" gate="G$1" pin="1"/>
<pinref part="SUPPLY69" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY5" gate="GND" pin="GND"/>
<pinref part="IC3" gate="G$1" pin="GND1"/>
<pinref part="IC3" gate="G$1" pin="PAD"/>
<pinref part="IC3" gate="G$1" pin="GND2"/>
<pinref part="C28" gate="G$1" pin="2"/>
<pinref part="C30" gate="G$1" pin="2"/>
<pinref part="C29" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="SUPPLY6" gate="GND" pin="GND"/>
<pinref part="R33" gate="G$1" pin="1"/>
<pinref part="R34" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY7" gate="GND" pin="GND"/>
<pinref part="R27" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C16" gate="G$1" pin="1"/>
<pinref part="SUPPLY8" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY9" gate="GND" pin="GND"/>
<pinref part="IC5" gate="G$1" pin="GND1"/>
<pinref part="IC5" gate="G$1" pin="PAD"/>
<pinref part="IC5" gate="G$1" pin="GND2"/>
<pinref part="C38" gate="G$1" pin="2"/>
<pinref part="C40" gate="G$1" pin="2"/>
<pinref part="C39" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="SUPPLY10" gate="GND" pin="GND"/>
<pinref part="R46" gate="G$1" pin="1"/>
<pinref part="R47" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY11" gate="GND" pin="GND"/>
<pinref part="R40" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C32" gate="G$1" pin="1"/>
<pinref part="SUPPLY12" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY13" gate="GND" pin="GND"/>
<pinref part="IC6" gate="G$1" pin="GND1"/>
<pinref part="IC6" gate="G$1" pin="PAD"/>
<pinref part="IC6" gate="G$1" pin="GND2"/>
<pinref part="C41" gate="G$1" pin="2"/>
<pinref part="C43" gate="G$1" pin="2"/>
<pinref part="C42" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="SUPPLY14" gate="GND" pin="GND"/>
<pinref part="R48" gate="G$1" pin="1"/>
<pinref part="R49" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY15" gate="GND" pin="GND"/>
<pinref part="R43" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C33" gate="G$1" pin="1"/>
<pinref part="SUPPLY16" gate="GND" pin="GND"/>
</segment>
</net>
<net name="STP1">
<segment>
<pinref part="IC2" gate="G$1" pin="STEP"/>
</segment>
</net>
<net name="P0W">
<segment>
<pinref part="IC4" gate="G$1" pin="P0W"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="REF"/>
</segment>
</net>
<net name="P1W">
<segment>
<pinref part="IC4" gate="G$1" pin="P1W"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="REF"/>
</segment>
</net>
<net name="P2W">
<segment>
<pinref part="IC4" gate="G$1" pin="P2W"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="REF"/>
</segment>
</net>
<net name="P3W">
<segment>
<pinref part="IC4" gate="G$1" pin="P3W"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="REF"/>
</segment>
</net>
<net name="TH1">
<segment>
<pinref part="C21" gate="G$1" pin="+"/>
<pinref part="SL1" gate="G$1" pin="2"/>
<pinref part="RN1" gate="A" pin="2"/>
</segment>
</net>
<net name="TH2">
<segment>
<pinref part="C22" gate="G$1" pin="+"/>
<pinref part="SL1" gate="G$1" pin="4"/>
<pinref part="RN1" gate="B" pin="2"/>
</segment>
</net>
<net name="TH3">
<segment>
<pinref part="C23" gate="G$1" pin="+"/>
<pinref part="SL1" gate="G$1" pin="6"/>
<pinref part="RN1" gate="C" pin="2"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="R37" gate="G$1" pin="1"/>
<pinref part="IC4" gate="G$1" pin="!RESET"/>
</segment>
</net>
<net name="N$90">
<segment>
<pinref part="IC2" gate="G$1" pin="CP1"/>
<pinref part="C19" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$93">
<segment>
<pinref part="IC2" gate="G$1" pin="CP2"/>
<pinref part="C19" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$96">
<segment>
<pinref part="C17" gate="G$1" pin="2"/>
<pinref part="IC2" gate="G$1" pin="VCP"/>
</segment>
</net>
<net name="N$98">
<segment>
<pinref part="IC2" gate="G$1" pin="SENSE1"/>
<pinref part="R31" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$99">
<segment>
<pinref part="IC2" gate="G$1" pin="SENSE2"/>
<pinref part="R32" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$101">
<segment>
<pinref part="IC2" gate="G$1" pin="OUT1A"/>
<pinref part="J1" gate="G$1" pin="2"/>
<pinref part="X1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$102">
<segment>
<pinref part="IC2" gate="G$1" pin="OUT1B"/>
<pinref part="J1" gate="G$1" pin="1"/>
<pinref part="X1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$103">
<segment>
<pinref part="IC2" gate="G$1" pin="OUT2A"/>
<pinref part="J1" gate="G$1" pin="3"/>
<pinref part="X1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$104">
<segment>
<pinref part="IC2" gate="G$1" pin="OUT2B"/>
<pinref part="J1" gate="G$1" pin="4"/>
<pinref part="X1" gate="G$1" pin="4"/>
</segment>
</net>
<net name="MS2">
<segment>
<pinref part="IC2" gate="G$1" pin="MS2"/>
<pinref part="JP30" gate="A" pin="1"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="MS2"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="MS2"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="MS2"/>
</segment>
</net>
<net name="MS1">
<segment>
<pinref part="IC2" gate="G$1" pin="MS1"/>
<pinref part="JP31" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="MS1"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="MS1"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="MS1"/>
</segment>
</net>
<net name="N$106">
<segment>
<pinref part="R26" gate="G$1" pin="1"/>
<pinref part="IC2" gate="G$1" pin="ROSC"/>
<pinref part="R22" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$107">
<segment>
<pinref part="IC2" gate="G$1" pin="VREG"/>
<pinref part="C15" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$108">
<segment>
<pinref part="R24" gate="G$1" pin="1"/>
<pinref part="IC2" gate="G$1" pin="^SLEEP"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="IC3" gate="G$1" pin="CP1"/>
<pinref part="C20" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="IC3" gate="G$1" pin="CP2"/>
<pinref part="C20" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="C18" gate="G$1" pin="2"/>
<pinref part="IC3" gate="G$1" pin="VCP"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="IC3" gate="G$1" pin="SENSE1"/>
<pinref part="R33" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="IC3" gate="G$1" pin="SENSE2"/>
<pinref part="R34" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="IC3" gate="G$1" pin="OUT1A"/>
<pinref part="J2" gate="G$1" pin="2"/>
<pinref part="X2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="IC3" gate="G$1" pin="OUT1B"/>
<pinref part="J2" gate="G$1" pin="1"/>
<pinref part="X2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="IC3" gate="G$1" pin="OUT2A"/>
<pinref part="J2" gate="G$1" pin="3"/>
<pinref part="X2" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="IC3" gate="G$1" pin="OUT2B"/>
<pinref part="J2" gate="G$1" pin="4"/>
<pinref part="X2" gate="G$1" pin="4"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="R27" gate="G$1" pin="1"/>
<pinref part="IC3" gate="G$1" pin="ROSC"/>
<pinref part="R23" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$22">
<segment>
<pinref part="IC3" gate="G$1" pin="VREG"/>
<pinref part="C16" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$24">
<segment>
<pinref part="IC3" gate="G$1" pin="^SLEEP"/>
<pinref part="R28" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$25">
<segment>
<pinref part="IC5" gate="G$1" pin="CP1"/>
<pinref part="C36" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$26">
<segment>
<pinref part="IC5" gate="G$1" pin="CP2"/>
<pinref part="C36" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$27">
<segment>
<pinref part="C34" gate="G$1" pin="2"/>
<pinref part="IC5" gate="G$1" pin="VCP"/>
</segment>
</net>
<net name="N$28">
<segment>
<pinref part="IC5" gate="G$1" pin="SENSE1"/>
<pinref part="R46" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$30">
<segment>
<pinref part="IC5" gate="G$1" pin="SENSE2"/>
<pinref part="R47" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$31">
<segment>
<pinref part="IC5" gate="G$1" pin="OUT1A"/>
<pinref part="J3" gate="G$1" pin="2"/>
<pinref part="X3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$32">
<segment>
<pinref part="IC5" gate="G$1" pin="OUT1B"/>
<pinref part="J3" gate="G$1" pin="1"/>
<pinref part="X3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$33">
<segment>
<pinref part="IC5" gate="G$1" pin="OUT2A"/>
<pinref part="J3" gate="G$1" pin="3"/>
<pinref part="X3" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$34">
<segment>
<pinref part="IC5" gate="G$1" pin="OUT2B"/>
<pinref part="J3" gate="G$1" pin="4"/>
<pinref part="X3" gate="G$1" pin="4"/>
</segment>
</net>
<net name="N$37">
<segment>
<pinref part="R40" gate="G$1" pin="1"/>
<pinref part="IC5" gate="G$1" pin="ROSC"/>
<pinref part="R38" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$38">
<segment>
<pinref part="IC5" gate="G$1" pin="VREG"/>
<pinref part="C32" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$40">
<segment>
<pinref part="IC5" gate="G$1" pin="^SLEEP"/>
<pinref part="R41" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$41">
<segment>
<pinref part="IC6" gate="G$1" pin="CP1"/>
<pinref part="C37" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$43">
<segment>
<pinref part="IC6" gate="G$1" pin="CP2"/>
<pinref part="C37" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$44">
<segment>
<pinref part="C35" gate="G$1" pin="2"/>
<pinref part="IC6" gate="G$1" pin="VCP"/>
</segment>
</net>
<net name="N$45">
<segment>
<pinref part="IC6" gate="G$1" pin="SENSE1"/>
<pinref part="R48" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$46">
<segment>
<pinref part="IC6" gate="G$1" pin="SENSE2"/>
<pinref part="R49" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$60">
<segment>
<pinref part="IC6" gate="G$1" pin="OUT1A"/>
<pinref part="J4" gate="G$1" pin="2"/>
<pinref part="X4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$48">
<segment>
<pinref part="IC6" gate="G$1" pin="OUT1B"/>
<pinref part="J4" gate="G$1" pin="1"/>
<pinref part="X4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$49">
<segment>
<pinref part="IC6" gate="G$1" pin="OUT2A"/>
<pinref part="J4" gate="G$1" pin="3"/>
<pinref part="X4" gate="G$1" pin="3"/>
</segment>
</net>
<net name="N$50">
<segment>
<pinref part="IC6" gate="G$1" pin="OUT2B"/>
<pinref part="J4" gate="G$1" pin="4"/>
<pinref part="X4" gate="G$1" pin="4"/>
</segment>
</net>
<net name="N$53">
<segment>
<pinref part="R43" gate="G$1" pin="1"/>
<pinref part="IC6" gate="G$1" pin="ROSC"/>
<pinref part="R39" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$54">
<segment>
<pinref part="IC6" gate="G$1" pin="VREG"/>
<pinref part="C33" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$57">
<segment>
<pinref part="IC6" gate="G$1" pin="^SLEEP"/>
<pinref part="R44" gate="G$1" pin="1"/>
</segment>
</net>
<net name="EN2">
<segment>
<pinref part="IC3" gate="G$1" pin="^EN"/>
</segment>
</net>
<net name="STP2">
<segment>
<pinref part="IC3" gate="G$1" pin="STEP"/>
</segment>
</net>
<net name="DIR2">
<segment>
<pinref part="IC3" gate="G$1" pin="DIR"/>
</segment>
</net>
<net name="EN3">
<segment>
<pinref part="IC5" gate="G$1" pin="^EN"/>
</segment>
</net>
<net name="STP3">
<segment>
<pinref part="IC5" gate="G$1" pin="STEP"/>
</segment>
</net>
<net name="DIR3">
<segment>
<pinref part="IC5" gate="G$1" pin="DIR"/>
</segment>
</net>
<net name="EN4">
<segment>
<pinref part="IC6" gate="G$1" pin="^EN"/>
</segment>
</net>
<net name="STP4">
<segment>
<pinref part="IC6" gate="G$1" pin="STEP"/>
</segment>
</net>
<net name="DIR4">
<segment>
<pinref part="IC6" gate="G$1" pin="DIR"/>
</segment>
</net>
<net name="TH4">
<segment>
<pinref part="C24" gate="G$1" pin="+"/>
<pinref part="SL1" gate="G$1" pin="8"/>
<pinref part="RN1" gate="D" pin="2"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="R30" gate="G$1" pin="1"/>
<pinref part="IC4" gate="G$1" pin="P3A"/>
<pinref part="IC4" gate="G$1" pin="P1A"/>
<pinref part="IC4" gate="G$1" pin="P0A"/>
<pinref part="IC4" gate="G$1" pin="P2A"/>
</segment>
</net>
<net name="POT_SCL">
<segment>
<pinref part="IC4" gate="G$1" pin="SCL"/>
<pinref part="R36" gate="G$1" pin="1"/>
</segment>
</net>
<net name="POT_SDA">
<segment>
<pinref part="IC4" gate="G$1" pin="SDA"/>
<pinref part="R35" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R25" gate="G$1" pin="1"/>
<pinref part="IC2" gate="G$1" pin="^RESET"/>
</segment>
</net>
<net name="N$35">
<segment>
<pinref part="R29" gate="G$1" pin="1"/>
<pinref part="IC3" gate="G$1" pin="^RESET"/>
</segment>
</net>
<net name="N$36">
<segment>
<pinref part="R42" gate="G$1" pin="1"/>
<pinref part="IC5" gate="G$1" pin="^RESET"/>
</segment>
</net>
<net name="N$39">
<segment>
<pinref part="R45" gate="G$1" pin="1"/>
<pinref part="IC6" gate="G$1" pin="^RESET"/>
</segment>
</net>
<net name="AVCC">
<segment>
<pinref part="RN1" gate="A" pin="1"/>
<pinref part="RN1" gate="B" pin="1"/>
<pinref part="RN1" gate="C" pin="1"/>
<pinref part="RN1" gate="D" pin="1"/>
</segment>
</net>
<net name="AGND">
<segment>
<pinref part="C21" gate="G$1" pin="-"/>
<pinref part="C22" gate="G$1" pin="-"/>
<pinref part="SL1" gate="G$1" pin="1"/>
<pinref part="SL1" gate="G$1" pin="3"/>
<pinref part="SL1" gate="G$1" pin="5"/>
<pinref part="SL1" gate="G$1" pin="7"/>
<pinref part="C23" gate="G$1" pin="-"/>
<pinref part="C24" gate="G$1" pin="-"/>
<pinref part="AGND3" gate="VR1" pin="AGND"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
<text>JP13,14   1-2: EXT FET- PS2</text>
<text>2-3: VBB </text>
<text>SMT FET PAIR</text>
<text>Small Power</text>
<text>TO220 FET PAIR</text>
<text>High Power</text>
<text>PWM Channel</text>
<text>GPIO Channel</text>
<text>GPIO Channel</text>
<text>PWM Channel</text>
<text>SmoothieBoard   ver 1.0</text>
<text>http://smoothieware.org</text>
</plain>
<busses>
</busses>
<nets>
<net name="N$42">
<segment>
<pinref part="IC8" gate="G$1" pin="RXD0"/>
<pinref part="R58" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$55">
<segment>
<pinref part="IC8" gate="G$1" pin="RXD1"/>
<pinref part="R59" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$63">
<segment>
<pinref part="IC8" gate="G$1" pin="CRS_DV"/>
<pinref part="R60" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ENET_TXD0">
<segment>
<pinref part="IC8" gate="G$1" pin="TXD0"/>
</segment>
</net>
<net name="ENET_TXD1">
<segment>
<pinref part="IC8" gate="G$1" pin="TXD1"/>
</segment>
</net>
<net name="ENET_TX_EN">
<segment>
<pinref part="IC8" gate="G$1" pin="TXEN"/>
</segment>
</net>
<net name="ENET_MDC">
<segment>
<pinref part="IC8" gate="G$1" pin="MDC"/>
</segment>
</net>
<net name="ENET_MDIO">
<segment>
<pinref part="IC8" gate="G$1" pin="MDIO"/>
<pinref part="R52" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ENET_RXD0">
<segment>
<pinref part="R58" gate="G$1" pin="2"/>
</segment>
</net>
<net name="ENET_RXD1">
<segment>
<pinref part="R59" gate="G$1" pin="2"/>
</segment>
</net>
<net name="ENET_CRS">
<segment>
<pinref part="R60" gate="G$1" pin="2"/>
</segment>
</net>
<net name="ENET_RX_ER">
<segment>
<pinref part="IC8" gate="G$1" pin="RXER"/>
<pinref part="R53" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$67">
<segment>
<pinref part="IC8" gate="G$1" pin="XTAL2"/>
<pinref part="C59" gate="G$1" pin="1"/>
<pinref part="R64" gate="G$1" pin="2"/>
<pinref part="Q3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$68">
<segment>
<pinref part="C58" gate="G$1" pin="1"/>
<pinref part="IC8" gate="G$1" pin="XTAL1"/>
<pinref part="R64" gate="G$1" pin="1"/>
<pinref part="Q3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="C58" gate="G$1" pin="2"/>
<pinref part="SUPPLY44" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C59" gate="G$1" pin="2"/>
<pinref part="SUPPLY45" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY43" gate="GND" pin="GND"/>
<pinref part="IC8" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R63" gate="G$1" pin="1"/>
<pinref part="SUPPLY46" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY47" gate="GND" pin="GND"/>
<pinref part="R62" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY48" gate="GND" pin="GND"/>
<pinref part="C45" gate="G$1" pin="-"/>
<pinref part="C47" gate="G$1" pin="2"/>
<pinref part="C46" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY49" gate="GND" pin="GND"/>
<pinref part="C51" gate="G$1" pin="2"/>
<pinref part="C50" gate="G$1" pin="-"/>
<pinref part="C48" gate="G$1" pin="-"/>
<pinref part="C49" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C54" gate="G$1" pin="2"/>
<pinref part="SUPPLY55" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C55" gate="G$1" pin="2"/>
<pinref part="SUPPLY54" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C56" gate="G$1" pin="2"/>
<pinref part="SUPPLY53" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C57" gate="G$1" pin="2"/>
<pinref part="SUPPLY52" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C52" gate="G$1" pin="2"/>
<pinref part="SUPPLY50" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="C53" gate="G$1" pin="2"/>
<pinref part="SUPPLY51" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="IC7" gate="G$1" pin="GND"/>
<pinref part="SUPPLY56" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="SUPPLY57" gate="GND" pin="GND"/>
<pinref part="C44" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC10" gate="G$1" pin="ADJ"/>
<pinref part="SUPPLY59" gate="GND" pin="GND"/>
<pinref part="C64" gate="G$1" pin="-"/>
<pinref part="C65" gate="G$1" pin="2"/>
<pinref part="LED9" gate="G$1" pin="C"/>
</segment>
<segment>
<pinref part="SUPPLY60" gate="GND" pin="GND"/>
<pinref part="X12" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="Q7" gate="G$1" pin="S"/>
<pinref part="Q6" gate="G$1" pin="S"/>
<pinref part="SUPPLY22" gate="GND" pin="GND"/>
<pinref part="Q8" gate="G$1" pin="S"/>
<pinref part="Q9" gate="G$1" pin="S"/>
<pinref part="R74" gate="G$1" pin="2"/>
<pinref part="R76" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY23" gate="GND" pin="GND"/>
<pinref part="C61" gate="G$1" pin="-"/>
<pinref part="X6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY24" gate="GND" pin="GND"/>
<pinref part="C60" gate="G$1" pin="-"/>
<pinref part="U$5" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="SUPPLY63" gate="GND" pin="GND"/>
<pinref part="LED10" gate="G$1" pin="C"/>
<pinref part="C63" gate="G$1" pin="-"/>
<pinref part="J10" gate="G$1" pin="PWR"/>
<pinref part="X11" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SUPPLY35" gate="GND" pin="GND"/>
<pinref part="POWER" gate="G$1" pin="GND"/>
<pinref part="POWER" gate="G$1" pin="GND1"/>
</segment>
<segment>
<pinref part="SUPPLY19" gate="GND" pin="GND"/>
<pinref part="RJ1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R61" gate="G$1" pin="1"/>
<pinref part="SUPPLY70" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="R50" gate="G$1" pin="1"/>
<pinref part="SUPPLY18" gate="GND" pin="GND"/>
</segment>
<segment>
<pinref part="RJ1" gate="G$1" pin="SHIELD1"/>
<pinref part="SUPPLY62" gate="GND" pin="GND"/>
<pinref part="RJ1" gate="G$1" pin="SHIELD0"/>
</segment>
<segment>
<pinref part="SUPPLY71" gate="GND" pin="GND"/>
<pinref part="R71" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SUPPLY73" gate="GND" pin="GND"/>
<pinref part="C62" gate="G$1" pin="2"/>
<pinref part="IC11" gate="G$1" pin="GND"/>
<pinref part="IC11" gate="G$1" pin="GND@1"/>
</segment>
<segment>
<pinref part="SUPPLY72" gate="GND" pin="GND"/>
<pinref part="C66" gate="G$1" pin="2"/>
<pinref part="U$2" gate="RAILS" pin="P$2"/>
</segment>
<segment>
<pinref part="R72" gate="G$1" pin="1"/>
<pinref part="SUPPLY78" gate="GND" pin="GND"/>
</segment>
</net>
<net name="N$69">
<segment>
<pinref part="IC8" gate="G$1" pin="RBIAS"/>
<pinref part="R63" gate="G$1" pin="2"/>
</segment>
</net>
<net name="LED1/REGOFF">
<segment>
<pinref part="IC8" gate="G$1" pin="LED1/REGOFF"/>
</segment>
<segment>
<pinref part="RJ1" gate="G$1" pin="G+"/>
</segment>
</net>
<net name="LED2/NINTSEL">
<segment>
<pinref part="IC8" gate="G$1" pin="LED2/NINTSEL"/>
<pinref part="R62" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="RJ1" gate="G$1" pin="Y+"/>
</segment>
</net>
<net name="3.3V">
<segment>
<pinref part="P+10" gate="G$1" pin="3.3V"/>
<pinref part="R52" gate="G$1" pin="2"/>
<pinref part="FB1" gate="G$1" pin="P$1"/>
<pinref part="R53" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC8" gate="G$1" pin="VDDIO"/>
<pinref part="P+14" gate="G$1" pin="3.3V"/>
<pinref part="C50" gate="G$1" pin="+"/>
<pinref part="C51" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+18" gate="G$1" pin="3.3V"/>
<pinref part="C44" gate="G$1" pin="1"/>
<pinref part="IC7" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="C65" gate="G$1" pin="1"/>
<pinref part="P+27" gate="G$1" pin="3.3V"/>
<pinref part="IC10" gate="G$1" pin="OUT"/>
<pinref part="IC10" gate="G$1" pin="OUT@1"/>
<pinref part="R77" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$82">
<segment>
<pinref part="IC8" gate="G$1" pin="VDDCR"/>
<pinref part="C49" gate="G$1" pin="1"/>
<pinref part="C48" gate="G$1" pin="+"/>
</segment>
</net>
<net name="TD+">
<segment>
<pinref part="IC8" gate="G$1" pin="TX+"/>
<pinref part="C54" gate="G$1" pin="1"/>
<pinref part="RJ1" gate="G$1" pin="TD+"/>
<pinref part="R54" gate="G$1" pin="2"/>
</segment>
</net>
<net name="TD-">
<segment>
<pinref part="IC8" gate="G$1" pin="TX-"/>
<pinref part="C55" gate="G$1" pin="1"/>
<pinref part="RJ1" gate="G$1" pin="TD-"/>
<pinref part="R55" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RD+">
<segment>
<pinref part="IC8" gate="G$1" pin="RX+"/>
<pinref part="C56" gate="G$1" pin="1"/>
<pinref part="RJ1" gate="G$1" pin="RD+"/>
<pinref part="R56" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RD-">
<segment>
<pinref part="IC8" gate="G$1" pin="RX-"/>
<pinref part="C57" gate="G$1" pin="1"/>
<pinref part="RJ1" gate="G$1" pin="RD-"/>
<pinref part="R57" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$77">
<segment>
<pinref part="IC8" gate="G$1" pin="NINT/REFCLKO"/>
<pinref part="IC7" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$78">
<segment>
<pinref part="IC7" gate="G$1" pin="Y"/>
<pinref part="R51" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ENET_REF_CLK">
<segment>
<pinref part="R51" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RSTOUT">
<segment>
<pinref part="IC8" gate="G$1" pin="NRST"/>
</segment>
</net>
<net name="5V">
<segment>
<pinref part="IC10" gate="G$1" pin="IN"/>
<pinref part="C64" gate="G$1" pin="+"/>
<pinref part="D1" gate="G$1" pin="C"/>
<pinref part="D2" gate="G$1" pin="C"/>
<pinref part="U$3" gate="G$1" pin="5V"/>
</segment>
</net>
<net name="VUSB">
<segment>
<pinref part="VUSB2" gate="G$1" pin="5V"/>
<pinref part="D1" gate="G$1" pin="A"/>
</segment>
</net>
<net name="+5V">
<segment>
<pinref part="D2" gate="G$1" pin="A"/>
<pinref part="X12" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="POWER" gate="G$1" pin="+5V"/>
</segment>
</net>
<net name="N$80">
<segment>
<pinref part="R77" gate="G$1" pin="1"/>
<pinref part="LED9" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$88">
<segment>
<pinref part="Q8" gate="G$1" pin="D"/>
<pinref part="J8" gate="G$1" pin="1"/>
<pinref part="LED5" gate="G$1" pin="C"/>
<pinref part="X7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$52">
<segment>
<pinref part="Q9" gate="G$1" pin="D"/>
<pinref part="X8" gate="G$1" pin="2"/>
<pinref part="J6" gate="G$1" pin="2"/>
<pinref part="LED6" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$92">
<segment>
<pinref part="Q6" gate="G$1" pin="D"/>
<pinref part="X10" gate="G$1" pin="1"/>
<pinref part="J9" gate="G$1" pin="1"/>
<pinref part="LED7" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$94">
<segment>
<pinref part="Q7" gate="G$1" pin="D"/>
<pinref part="LED8" gate="G$1" pin="C"/>
<pinref part="U$6" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="VBB">
<segment>
<pinref part="R78" gate="G$1" pin="2"/>
<pinref part="C63" gate="G$1" pin="+"/>
<pinref part="U$1" gate="G$1" pin="K"/>
</segment>
<segment>
<pinref part="JP28" gate="A" pin="2"/>
</segment>
<segment>
<pinref part="JP11" gate="A" pin="2"/>
<pinref part="JP27" gate="A" pin="2"/>
</segment>
</net>
<net name="N$74">
<segment>
<pinref part="R73" gate="G$1" pin="1"/>
<pinref part="Q8" gate="G$1" pin="G"/>
</segment>
</net>
<net name="N$75">
<segment>
<pinref part="R75" gate="G$1" pin="1"/>
<pinref part="Q9" gate="G$1" pin="G"/>
</segment>
</net>
<net name="MOSFET_DRIVE">
<segment>
<pinref part="C60" gate="G$1" pin="+"/>
<pinref part="JP11" gate="A" pin="1"/>
<pinref part="JP27" gate="A" pin="1"/>
<pinref part="X10" gate="G$1" pin="2"/>
<pinref part="J9" gate="G$1" pin="2"/>
<pinref part="R67" gate="G$1" pin="1"/>
<pinref part="R68" gate="G$1" pin="1"/>
<pinref part="U$5" gate="G$1" pin="P$1"/>
<pinref part="U$6" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="IC11" gate="G$1" pin="VI"/>
</segment>
</net>
<net name="N$18">
<segment>
<pinref part="X6" gate="G$1" pin="1"/>
<pinref part="JP28" gate="A" pin="1"/>
<pinref part="C61" gate="G$1" pin="+"/>
<pinref part="X8" gate="G$1" pin="1"/>
<pinref part="J6" gate="G$1" pin="1"/>
<pinref part="J8" gate="G$1" pin="2"/>
<pinref part="R65" gate="G$1" pin="1"/>
<pinref part="R66" gate="G$1" pin="1"/>
<pinref part="X7" gate="G$1" pin="1"/>
</segment>
</net>
<net name="PWM0">
<segment>
<pinref part="R73" gate="G$1" pin="2"/>
<pinref part="R74" gate="G$1" pin="1"/>
</segment>
</net>
<net name="P2.6">
<segment>
<pinref part="R75" gate="G$1" pin="2"/>
<pinref part="R76" gate="G$1" pin="1"/>
</segment>
</net>
<net name="P2.7">
<segment>
<pinref part="R72" gate="G$1" pin="2"/>
<pinref part="U$2" gate="B" pin="P$1"/>
</segment>
</net>
<net name="N$16">
<segment>
<pinref part="R78" gate="G$1" pin="1"/>
<pinref part="LED10" gate="G$1" pin="A"/>
</segment>
</net>
<net name="VBB_IN">
<segment>
<pinref part="J10" gate="G$1" pin="GND"/>
<pinref part="X11" gate="G$1" pin="1"/>
<pinref part="U$1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="POWER" gate="G$1" pin="+12V"/>
</segment>
</net>
<net name="N$81">
<segment>
<pinref part="R65" gate="G$1" pin="2"/>
<pinref part="LED5" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$91">
<segment>
<pinref part="R66" gate="G$1" pin="2"/>
<pinref part="LED6" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$105">
<segment>
<pinref part="R67" gate="G$1" pin="2"/>
<pinref part="LED7" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$112">
<segment>
<pinref part="R68" gate="G$1" pin="2"/>
<pinref part="LED8" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$20">
<segment>
<pinref part="RJ1" gate="G$1" pin="G-"/>
<pinref part="R61" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$47">
<segment>
<pinref part="RJ1" gate="G$1" pin="Y-"/>
<pinref part="R50" gate="G$1" pin="2"/>
</segment>
</net>
<net name="12VREG">
<segment>
<pinref part="C62" gate="G$1" pin="1"/>
<pinref part="C66" gate="G$1" pin="1"/>
<pinref part="U$2" gate="RAILS" pin="P$1"/>
<pinref part="IC11" gate="G$1" pin="VO"/>
</segment>
</net>
<net name="PWM1_FET">
<segment>
<pinref part="R69" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="Q6" gate="G$1" pin="G"/>
</segment>
</net>
<net name="GPIO_FET">
<segment>
<pinref part="R70" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="Q7" gate="G$1" pin="G"/>
</segment>
</net>
<net name="PWM1">
<segment>
<pinref part="R71" gate="G$1" pin="2"/>
<pinref part="U$2" gate="A" pin="P$1"/>
</segment>
</net>
<net name="N$21">
<segment>
<pinref part="RJ1" gate="G$1" pin="P4"/>
<pinref part="RJ1" gate="G$1" pin="P5"/>
<pinref part="C53" gate="G$1" pin="1"/>
<pinref part="FB1" gate="G$1" pin="P$2"/>
<pinref part="IC8" gate="G$1" pin="VDD2A"/>
<pinref part="IC8" gate="G$1" pin="VDD1A"/>
<pinref part="C47" gate="G$1" pin="1"/>
<pinref part="C46" gate="G$1" pin="1"/>
<pinref part="C45" gate="G$1" pin="+"/>
<pinref part="C52" gate="G$1" pin="1"/>
<pinref part="R54" gate="G$1" pin="1"/>
<pinref part="R55" gate="G$1" pin="1"/>
<pinref part="R56" gate="G$1" pin="1"/>
<pinref part="R57" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="R69" gate="G$1" pin="1"/>
<pinref part="U$2" gate="A" pin="P$2"/>
</segment>
</net>
<net name="N$19">
<segment>
<pinref part="U$2" gate="B" pin="P$2"/>
<pinref part="R70" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
